#!/bin/sh /etc/rc.common
#
# Copyright (C) 2011 OpenWrt.org
#

START=11
STOP=11

USE_PROCD=1
NAME=om-watchdog
PROG=/sbin/om-watchdog

get_gpio() {
	if [ -r /lib/ar71xx.sh ]; then
		. /lib/ar71xx.sh
		local board=$(ar71xx_board_name)

		case "$board" in
			"om2p" | \
			"om2pv4" | \
			"om2p-hs" | \
			"om2p-hsv2" | \
			"om2p-hsv3" | \
			"om2p-hsv4" | \
			"om5p-acv2")
				return 12
				;;
			"om2pv2" | \
			"om2p-lc")
				return 26
				;;
			"om5p" | \
			"om5p-an")
				return 11
				;;
			"om5p-ac")
				return 17
				;;
			"mr600v2")
				return 15
				;;
			"mr900" | \
			"mr900v2" | \
			"mr1750" | \
			"mr1750v2" | \
			"a40" | \
			"a60")
				return 16
				;;
		esac
	else
		#we assume it is om1p in this case
		return 3
	fi

	return 255
}

start_service() {
	get_gpio
	gpio="$?"
	[ "$gpio" != "255" ] || return

	procd_open_instance
	procd_set_param command "${PROG}" "${gpio}"
	procd_set_param respawn
	procd_close_instance
}
