From d532c1082f68176363ed766d09bf187616e282fe Mon Sep 17 00:00:00 2001
From: Eric Dumazet <edumazet@google.com>
Date: Wed, 19 Apr 2017 09:59:23 -0700
Subject: [PATCH] sr9700: use skb_cow_head() to deal with cloned skbs

We need to ensure there is enough headroom to push extra header,
but we also need to check if we are allowed to change headers.

skb_cow_head() is the proper helper to deal with this.

Fixes: c9b37458e956 ("USB2NET : SR9700 : One chip USB 1.1 USB2NET SR9700Device Driver Support")
Signed-off-by: Eric Dumazet <edumazet@google.com>
Cc: James Hughes <james.hughes@raspberrypi.org>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/usb/sr9700.c | 9 ++-------
 1 file changed, 2 insertions(+), 7 deletions(-)

--- a/drivers/net/usb/sr9700.c
+++ b/drivers/net/usb/sr9700.c
@@ -456,14 +456,9 @@ static struct sk_buff *sr9700_tx_fixup(s
 
 	len = skb->len;
 
-	if (skb_headroom(skb) < SR_TX_OVERHEAD) {
-		struct sk_buff *skb2;
-
-		skb2 = skb_copy_expand(skb, SR_TX_OVERHEAD, 0, flags);
+	if (skb_cow_head(skb, SR_TX_OVERHEAD)) {
 		dev_kfree_skb_any(skb);
-		skb = skb2;
-		if (!skb)
-			return NULL;
+		return NULL;
 	}
 
 	__skb_push(skb, SR_TX_OVERHEAD);
