From eef9dfc4e821408af1af13aa0cc707fc496fb7c6 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Wed, 11 Dec 2013 19:05:59 +0100
Subject: [PATCH] m25p80: add support for the Winbond W25X05 flash

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/mtd/devices/m25p80.c |    1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -618,6 +618,7 @@ static const struct spi_device_id spi_no
 	{ "m25px80",    INFO(0x207114,  0, 64 * 1024, 16, 0) },
 
 	/* Winbond -- w25x "blocks" are 64K, "sectors" are 4KiB */
+	{ "w25x05", INFO(0xef3010, 0, 64 * 1024,  1,  SECT_4K) },
 	{ "w25x10", INFO(0xef3011, 0, 64 * 1024,  2,  SECT_4K) },
 	{ "w25x20", INFO(0xef3012, 0, 64 * 1024,  4,  SECT_4K) },
 	{ "w25x40", INFO(0xef3013, 0, 64 * 1024,  8,  SECT_4K) },
