From dd35cc0896faff5ed9d22eac9ea4a1920e2eec0c Mon Sep 17 00:00:00 2001
From: Stanislaw Gruszka <sgruszka@redhat.com>
Date: Wed, 15 Feb 2017 10:25:13 +0100
Subject: [PATCH 17/19] rt2x00: fix rt2x00debug_dump_frame comment

Reported-by: Jeroen Roovers <jer@airfi.aero>
Signed-off-by: Stanislaw Gruszka <sgruszka@redhat.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2x00.h | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/net/wireless/ralink/rt2x00/rt2x00.h b/drivers/net/wireless/ralink/rt2x00/rt2x00.h
index 91ba10fdf732..ce340bfd71a0 100644
--- a/drivers/net/wireless/ralink/rt2x00/rt2x00.h
+++ b/drivers/net/wireless/ralink/rt2x00/rt2x00.h
@@ -1396,7 +1396,7 @@ void rt2x00queue_flush_queues(struct rt2x00_dev *rt2x00dev, bool drop);
  * rt2x00debug_dump_frame - Dump a frame to userspace through debugfs.
  * @rt2x00dev: Pointer to &struct rt2x00_dev.
  * @type: The type of frame that is being dumped.
- * @skb: The skb containing the frame to be dumped.
+ * @entry: The queue entry containing the frame to be dumped.
  */
 #ifdef CPTCFG_RT2X00_LIB_DEBUGFS
 void rt2x00debug_dump_frame(struct rt2x00_dev *rt2x00dev,
-- 
2.12.1

