From 11c40fb47c4a4dd6ad060c2ae127ced89ffb9fe1 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Thu, 18 Apr 2013 14:33:33 +0200
Subject: [PATCH] rt2x00: rt2800lib: use correct [RT]XWI size for RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |    1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -587,6 +587,7 @@ void rt2800_get_txwi_rxwi_size(struct rt
 {
 	switch (rt2x00dev->chip.rt) {
 	case RT3593:
+	case RT3883:
 		*txwi_size = TXWI_DESC_SIZE_4WORDS;
 		*rxwi_size = RXWI_DESC_SIZE_5WORDS;
 		break;
