From 1bd1b740f208d1cf4071932cc51860d37266c402 Mon Sep 17 00:00:00 2001
From: Bernhard Frauendienst <kernel@nospam.obeliks.de>
Date: Sat, 1 Sep 2018 00:30:11 +0200
Subject: [PATCH 495/497] mtd: core: add get_mtd_device_by_node

Add function to retrieve a mtd device by its OF node. Since drivers can
assign arbitrary names to mtd devices in the absence of a label
property, there is no other reliable way to retrieve a mtd device for a
given OF node.

Signed-off-by: Bernhard Frauendienst <kernel@nospam.obeliks.de>
Reviewed-by: Miquel Raynal <miquel.raynal@bootlin.com>
---
 drivers/mtd/mtdcore.c   | 38 ++++++++++++++++++++++++++++++++++++++
 include/linux/mtd/mtd.h |  2 ++
 2 files changed, 40 insertions(+)

--- a/drivers/mtd/mtdcore.c
+++ b/drivers/mtd/mtdcore.c
@@ -926,6 +926,44 @@ out_unlock:
 }
 EXPORT_SYMBOL_GPL(get_mtd_device_nm);
 
+/**
+ *	get_mtd_device_by_node - obtain a validated handle for an MTD device
+ *	by of_node
+ *	@of_node: OF node of MTD device to open
+ *
+ *	This function returns MTD device description structure in case of
+ *	success and an error code in case of failure.
+ */
+struct mtd_info *get_mtd_device_by_node(const struct device_node *of_node)
+{
+	int err = -ENODEV;
+	struct mtd_info *mtd = NULL, *other;
+
+	mutex_lock(&mtd_table_mutex);
+
+	mtd_for_each_device(other) {
+		if (of_node == other->dev.of_node) {
+			mtd = other;
+			break;
+		}
+	}
+
+	if (!mtd)
+		goto out_unlock;
+
+	err = __get_mtd_device(mtd);
+	if (err)
+		goto out_unlock;
+
+	mutex_unlock(&mtd_table_mutex);
+	return mtd;
+
+out_unlock:
+	mutex_unlock(&mtd_table_mutex);
+	return ERR_PTR(err);
+}
+EXPORT_SYMBOL_GPL(get_mtd_device_by_node);
+
 void put_mtd_device(struct mtd_info *mtd)
 {
 	mutex_lock(&mtd_table_mutex);
--- a/include/linux/mtd/mtd.h
+++ b/include/linux/mtd/mtd.h
@@ -580,6 +580,8 @@ extern struct mtd_info *get_mtd_device(s
 extern int __get_mtd_device(struct mtd_info *mtd);
 extern void __put_mtd_device(struct mtd_info *mtd);
 extern struct mtd_info *get_mtd_device_nm(const char *name);
+extern struct mtd_info *get_mtd_device_by_node(
+		const struct device_node *of_node);
 extern void put_mtd_device(struct mtd_info *mtd);
 
 
