--- a/arch/arm/dts/Makefile
+++ b/arch/arm/dts/Makefile
@@ -107,6 +107,7 @@ dtb-$(CONFIG_ROCKCHIP_RK3308) += \
 dtb-$(CONFIG_ROCKCHIP_RK3328) += \
 	rk3328-evb.dtb \
 	rk3328-nanopi-r2s.dtb \
+	rk3328-tpe-r1400.dtb \
 	rk3328-roc-cc.dtb \
 	rk3328-rock64.dtb \
 	rk3328-rock-pi-e.dtb
--- /dev/null
+++ b/arch/arm/dts/rk3328-tpe-r1400-u-boot.dtsi
@@ -0,0 +1,34 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * (C) Copyright 2018-2019 Rockchip Electronics Co., Ltd
+ * (C) Copyright 2020 David Bauer
+ */
+
+#include "rk3328-u-boot.dtsi"
+#include "rk3328-sdram-ddr4-666.dtsi"
+/ {
+	chosen {
+		u-boot,spl-boot-order = "same-as-spl", &sdmmc, &emmc;
+	};
+};
+
+&gpio0 {
+	u-boot,dm-spl;
+};
+
+&pinctrl {
+	u-boot,dm-spl;
+};
+
+&sdmmc0m1_gpio {
+	u-boot,dm-spl;
+};
+
+&pcfg_pull_up_4ma {
+	u-boot,dm-spl;
+};
+
+/* Need this and all the pinctrl/gpio stuff above to set pinmux */
+&vcc_sd {
+	u-boot,dm-spl;
+};
--- /dev/null
+++ b/arch/arm/dts/rk3328-tpe-r1400.dts
@@ -0,0 +1,334 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright (c) 2020 David Bauer <mail@david-bauer.net>
+ */
+
+/dts-v1/;
+
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/gpio/gpio.h>
+#include "rk3328.dtsi"
+
+/ {
+	model = "ThinkPenguin TPE-R1400";
+	compatible = "thinkpenguin,tpe-r1400", "rockchip,rk3328";
+
+	chosen {
+		stdout-path = "serial2:1500000n8";
+	};
+
+	gmac_clkin: external-gmac-clock {
+		compatible = "fixed-clock";
+		clock-frequency = <125000000>;
+		clock-output-names = "gmac_clkin";
+		#clock-cells = <0>;
+	};
+
+	vcc_sd: sdmmc-regulator {
+		compatible = "regulator-fixed";
+		gpio = <&gpio0 RK_PD6 GPIO_ACTIVE_LOW>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&sdmmc0m1_gpio>;
+		regulator-name = "vcc_sd";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc_io>;
+	};
+
+	vcc_sdio: sdmmcio-regulator {
+		compatible = "regulator-gpio";
+		gpios = <&gpio1 RK_PD4 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+		states = <1800000 0x1
+			  3300000 0x0>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&sdio_vcc_pin>;
+		regulator-always-on;
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-name = "vcc_sdio";
+		regulator-settling-time-us = <5000>;
+		regulator-type = "voltage";
+		vin-supply = <&vcc_io>;
+	};
+
+	vcc_sys: vcc-sys {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pinctrl-names = "default";
+		pinctrl-0 = <&led_pins>;
+
+		sys {
+			gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_HIGH>;
+			label = "tpe-r1400:red:sys";
+		};
+
+		lan {
+			gpios = <&gpio2 RK_PB7 GPIO_ACTIVE_HIGH>;
+			label = "tpe-r1400:green:lan";
+		};
+
+		wan {
+			gpios = <&gpio2 RK_PC2 GPIO_ACTIVE_HIGH>;
+			label = "tpe-r1400:green:wan";
+		};
+	};
+
+	gpio_keys {
+		compatible = "gpio-keys-polled";
+		poll-interval = <100>;
+
+		pinctrl-names = "default";
+		pinctrl-0 = <&button_pins>;
+
+		reset {
+			label = "Reset Button";
+			gpios = <&gpio0 RK_PA0 GPIO_ACTIVE_LOW>;
+			linux,code = <KEY_RESTART>;
+			debounce-interval = <50>;
+		};
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu1 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu2 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu3 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&gmac2io {
+	assigned-clocks = <&cru SCLK_MAC2IO>, <&cru SCLK_MAC2IO_EXT>;
+	assigned-clock-parents = <&gmac_clkin>, <&gmac_clkin>;
+	clock_in_out = "input";
+	phy-supply = <&vcc_io>;
+	phy-handle = <&rtl8211e>;
+	phy-mode = "rgmii";
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmiim1_pins>;
+	snps,aal;
+	snps,reset-gpio = <&gpio1 RK_PC2 GPIO_ACTIVE_LOW>;
+	snps,reset-active-low;
+	snps,reset-delays-us = <0 10000 50000>;
+	tx_delay = <0x24>;
+	rx_delay = <0x18>;
+	status = "okay";
+
+	mdio {
+		compatible = "snps,dwmac-mdio";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		rtl8211e: ethernet-phy@0 {
+			reg = <0>;
+		};
+	};
+};
+
+&i2c1 {
+	status = "okay";
+
+	rk805: rk805@18 {
+		compatible = "rockchip,rk805";
+		reg = <0x18>;
+		interrupt-parent = <&gpio2>;
+		interrupts = <6 IRQ_TYPE_LEVEL_LOW>;
+		#clock-cells = <1>;
+		clock-output-names = "xin32k", "rk805-clkout2";
+		gpio-controller;
+		#gpio-cells = <2>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pmic_int_l>;
+		rockchip,system-power-controller;
+		wakeup-source;
+
+		vcc1-supply = <&vcc_sys>;
+		vcc2-supply = <&vcc_sys>;
+		vcc3-supply = <&vcc_sys>;
+		vcc4-supply = <&vcc_sys>;
+		vcc5-supply = <&vcc_io>;
+		vcc6-supply = <&vcc_sys>;
+
+		regulators {
+			vdd_logic: DCDC_REG1 {
+				regulator-name = "vdd_logic";
+				regulator-min-microvolt = <712500>;
+				regulator-max-microvolt = <1450000>;
+				regulator-ramp-delay = <12500>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1000000>;
+				};
+			};
+
+			vdd_arm: DCDC_REG2 {
+				regulator-name = "vdd_arm";
+				regulator-min-microvolt = <712500>;
+				regulator-max-microvolt = <1450000>;
+				regulator-ramp-delay = <12500>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <950000>;
+				};
+			};
+
+			vcc_ddr: DCDC_REG3 {
+				regulator-name = "vcc_ddr";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+				};
+			};
+
+			vcc_io: DCDC_REG4 {
+				regulator-name = "vcc_io";
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3300000>;
+				};
+			};
+
+			vcc_18: LDO_REG1 {
+				regulator-name = "vcc_18";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vcc18_emmc: LDO_REG2 {
+				regulator-name = "vcc18_emmc";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vdd_10: LDO_REG3 {
+				regulator-name = "vdd_10";
+				regulator-min-microvolt = <1000000>;
+				regulator-max-microvolt = <1000000>;
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1000000>;
+				};
+			};
+		};
+	};
+};
+
+&io_domains {
+	status = "okay";
+
+	vccio1-supply = <&vcc_io>;
+	vccio2-supply = <&vcc18_emmc>;
+	vccio3-supply = <&vcc_sdio>;
+	vccio4-supply = <&vcc_18>;
+	vccio5-supply = <&vcc_io>;
+	vccio6-supply = <&vcc_io>;
+	pmuio-supply = <&vcc_io>;
+};
+
+&pinctrl {
+	leds {
+		led_pins: led-pins {
+			rockchip,pins = <0 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>,
+							<2 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>,
+							<2 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	button {
+		button_pins: button-pins {
+			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	pmic {
+		pmic_int_l: pmic-int-l {
+			rockchip,pins = <2 RK_PA6 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	sd {
+		sdio_vcc_pin: sdio-vcc-pin {
+			rockchip,pins = <1 RK_PD4 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+};
+
+&sdmmc {
+	bus-width = <4>;
+	cap-mmc-highspeed;
+	cap-sd-highspeed;
+	disable-wp;
+	max-frequency = <150000000>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdmmc0_clk &sdmmc0_cmd &sdmmc0_dectn &sdmmc0_bus4>;
+	vmmc-supply = <&vcc_sd>;
+	vqmmc-supply = <&vcc_sdio>;
+	status = "okay";
+};
+
+&tsadc {
+	rockchip,hw-tshut-mode = <0>;
+	rockchip,hw-tshut-polarity = <0>;
+	status = "okay";
+};
+
+&uart2 {
+	status = "okay";
+};
+
+&u2phy {
+	status = "okay";
+
+	u2phy_host: host-port {
+		status = "okay";
+	};
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
--- /dev/null
+++ b/configs/tpe-r1400-rk3328_defconfig
@@ -0,0 +1,99 @@
+CONFIG_ARM=y
+CONFIG_ARCH_ROCKCHIP=y
+CONFIG_SYS_TEXT_BASE=0x00200000
+CONFIG_SPL_GPIO_SUPPORT=y
+CONFIG_ENV_OFFSET=0x3F8000
+CONFIG_ROCKCHIP_RK3328=y
+CONFIG_TPL_ROCKCHIP_COMMON_BOARD=y
+CONFIG_TPL_LIBCOMMON_SUPPORT=y
+CONFIG_TPL_LIBGENERIC_SUPPORT=y
+CONFIG_SPL_DRIVERS_MISC_SUPPORT=y
+CONFIG_SPL_STACK_R_ADDR=0x600000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_DEBUG_UART_BASE=0xFF130000
+CONFIG_DEBUG_UART_CLOCK=24000000
+CONFIG_SMBIOS_PRODUCT_NAME="tpe_r1400_rk3328"
+CONFIG_DEBUG_UART=y
+CONFIG_TPL_SYS_MALLOC_F_LEN=0x800
+# CONFIG_ANDROID_BOOT_IMAGE is not set
+CONFIG_FIT=y
+CONFIG_FIT_VERBOSE=y
+CONFIG_SPL_LOAD_FIT=y
+CONFIG_DEFAULT_FDT_FILE="rockchip/rk3328-tpe-r1400.dtb"
+CONFIG_MISC_INIT_R=y
+# CONFIG_DISPLAY_CPUINFO is not set
+CONFIG_DISPLAY_BOARDINFO_LATE=y
+# CONFIG_SPL_RAW_IMAGE_SUPPORT is not set
+CONFIG_TPL_SYS_MALLOC_SIMPLE=y
+CONFIG_SPL_STACK_R=y
+CONFIG_SPL_I2C_SUPPORT=y
+CONFIG_SPL_POWER_SUPPORT=y
+CONFIG_SPL_ATF=y
+CONFIG_SPL_ATF_NO_PLATFORM_PARAM=y
+CONFIG_CMD_BOOTZ=y
+CONFIG_CMD_GPT=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_USB=y
+# CONFIG_CMD_SETEXPR is not set
+CONFIG_CMD_TIME=y
+CONFIG_SPL_OF_CONTROL=y
+CONFIG_TPL_OF_CONTROL=y
+CONFIG_DEFAULT_DEVICE_TREE="rk3328-tpe-r1400"
+CONFIG_OF_SPL_REMOVE_PROPS="clock-names interrupt-parent assigned-clocks assigned-clock-rates assigned-clock-parents"
+CONFIG_TPL_OF_PLATDATA=y
+CONFIG_ENV_IS_IN_MMC=y
+CONFIG_SYS_RELOC_GD_ENV_ADDR=y
+CONFIG_NET_RANDOM_ETHADDR=y
+CONFIG_TPL_DM=y
+CONFIG_REGMAP=y
+CONFIG_SPL_REGMAP=y
+CONFIG_TPL_REGMAP=y
+CONFIG_SYSCON=y
+CONFIG_SPL_SYSCON=y
+CONFIG_TPL_SYSCON=y
+CONFIG_CLK=y
+CONFIG_SPL_CLK=y
+CONFIG_FASTBOOT_BUF_ADDR=0x800800
+CONFIG_FASTBOOT_CMD_OEM_FORMAT=y
+CONFIG_ROCKCHIP_GPIO=y
+CONFIG_SYS_I2C_ROCKCHIP=y
+CONFIG_MMC_DW=y
+CONFIG_MMC_DW_ROCKCHIP=y
+CONFIG_SF_DEFAULT_SPEED=20000000
+CONFIG_DM_ETH=y
+CONFIG_ETH_DESIGNWARE=y
+CONFIG_GMAC_ROCKCHIP=y
+CONFIG_PINCTRL=y
+CONFIG_SPL_PINCTRL=y
+CONFIG_DM_PMIC=y
+CONFIG_PMIC_RK8XX=y
+CONFIG_SPL_DM_REGULATOR=y
+CONFIG_REGULATOR_PWM=y
+CONFIG_DM_REGULATOR_FIXED=y
+CONFIG_SPL_DM_REGULATOR_FIXED=y
+CONFIG_REGULATOR_RK8XX=y
+CONFIG_PWM_ROCKCHIP=y
+CONFIG_RAM=y
+CONFIG_SPL_RAM=y
+CONFIG_TPL_RAM=y
+CONFIG_DM_RESET=y
+CONFIG_BAUDRATE=1500000
+CONFIG_DEBUG_UART_SHIFT=2
+CONFIG_SYSRESET=y
+# CONFIG_TPL_SYSRESET is not set
+CONFIG_USB=y
+CONFIG_USB_XHCI_HCD=y
+CONFIG_USB_XHCI_DWC3=y
+CONFIG_USB_EHCI_HCD=y
+CONFIG_USB_EHCI_GENERIC=y
+CONFIG_USB_OHCI_HCD=y
+CONFIG_USB_OHCI_GENERIC=y
+CONFIG_USB_DWC2=y
+CONFIG_USB_DWC3=y
+# CONFIG_USB_DWC3_GADGET is not set
+CONFIG_USB_GADGET=y
+CONFIG_USB_GADGET_DWC2_OTG=y
+CONFIG_SPL_TINY_MEMSET=y
+CONFIG_TPL_TINY_MEMSET=y
+CONFIG_ERRNO_STR=y
+CONFIG_SMBIOS_MANUFACTURER="pine64"
