#!/bin/sh
#
# Copyright (C) 2014-2016 OpenWrt.org
# Copyright (C) 2016 LEDE-Project.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
cznic,turris-omnia)
	ucidef_set_interface_lan "lan0 lan1 lan2 lan3 lan4"
	ucidef_set_interface_wan "eth2"
	;;
globalscale,espressobin|\
globalscale,espressobin-emmc|\
globalscale,espressobin-v7|\
globalscale,espressobin-v7-emmc)
	ucidef_set_interfaces_lan_wan "lan0 lan1" "wan"
	;;
linksys,caiman|\
linksys,cobra|\
linksys,mamba|\
linksys,rango|\
linksys,shelby|\
linksys,venom)
	ucidef_set_interfaces_lan_wan "eth0.1" "eth1.2"
	ucidef_add_switch "switch0" \
		"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5@eth0" "4:wan" "6@eth1"
	;;
marvell,a385-db-ap)
	ucidef_set_interfaces_lan_wan "eth0 eth1" "eth2"
	;;
marvell,armada8040-mcbin)
	ucidef_set_interfaces_lan_wan "eth0 eth1 eth3" "eth2"
	;;
marvell,armada8040-db)
	ucidef_set_interfaces_lan_wan "eth0 eth2 eth3" "eth1"
	;;
marvell,armada7040-db)
	ucidef_set_interfaces_lan_wan "eth0 eth2" "eth1"
	;;
marvell,armada-3720-db)
	ucidef_set_interfaces_lan_wan "eth1" "eth0"
	;;
marvell,axp-gp)
	ucidef_set_interface_lan "eth0 eth1 eth2 eth3"
	;;
solidrun,clearfog*a1)
	# eth0 is standalone ethernet
	# eth1 is switch (-pro) or standalone ethernet (-base)
	# eth2 is SFP
	ucidef_set_interfaces_lan_wan "eth1" "eth0 eth2"

	# if switch exists (clearfog-pro)
	# switch port 5 is connected to eth1
	swconfig list 2>&1 | grep -q switch0 && \
		ucidef_add_switch "switch0" \
			"0:lan:5" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5u@eth1" "6:lan:6"
	;;
*)
	ucidef_set_interface_lan "eth0"
	;;
esac

board_config_flush

exit 0
