From 0c8856211d26f84277f7fcb0b9595e5c646bc464 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Tue, 6 Mar 2018 10:00:55 +0100
Subject: [PATCH 11/33] MIPS: ath79: select the PINCTRL subsystem

The pinmux on QCA SoCs is controlled by a single register. The
"pinctrl-single" driver can be used but requires the target
to select PINCTRL.

Signed-off-by: John Crispin <john@phrozen.org>
---
 arch/mips/Kconfig | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -193,6 +193,7 @@ config ATH79
 	select CSRC_R4K
 	select DMA_NONCOHERENT
 	select GPIOLIB
+	select PINCTRL
 	select HAVE_CLK
 	select COMMON_CLK
 	select CLKDEV_LOOKUP
