--- a/arch/arm/boot/dts/armada-385-linksys.dtsi
+++ b/arch/arm/boot/dts/armada-385-linksys.dtsi
@@ -196,6 +196,7 @@
 	status = "okay";
 
 	switch@0 {
+		status = "disabled";
 		compatible = "marvell,mv88e6085";
 		#address-cells = <1>;
 		#size-cells = <0>;
--- a/arch/arm/boot/dts/armada-388-clearfog.dts
+++ b/arch/arm/boot/dts/armada-388-clearfog.dts
@@ -202,6 +202,7 @@
 	status = "okay";
 
 	switch@4 {
+		status = "disabled";
 		compatible = "marvell,mv88e6085";
 		#address-cells = <1>;
 		#size-cells = <0>;
--- a/arch/arm/boot/dts/armada-xp-linksys-mamba.dts
+++ b/arch/arm/boot/dts/armada-xp-linksys-mamba.dts
@@ -516,6 +516,7 @@
 	status = "okay";
 
 	switch@0 {
+		status = "disabled";
 		compatible = "marvell,mv88e6085";
 		#address-cells = <1>;
 		#size-cells = <0>;
