From 4904337fe34fa7fc529d6f4d9ee8b96fe7db310a Mon Sep 17 00:00:00 2001
From: Corentin Labbe <clabbe.montjoie@gmail.com>
Date: Tue, 31 Oct 2017 09:19:12 +0100
Subject: [PATCH] ARM: dts: sunxi: Restore EMAC changes (boards)

The original dwmac-sun8i DT bindings have some issue on how to handle
integrated PHY and was reverted in last RC of 4.13.
But now we have a solution so we need to get back that was reverted.

This patch restore all boards DT about dwmac-sun8i
This reverts partially commit fe45174b72ae ("arm: dts: sunxi: Revert EMAC changes")

Signed-off-by: Corentin Labbe <clabbe.montjoie@gmail.com>
Acked-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun8i-h2-plus-orangepi-zero.dts |  9 +++++++
 arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts   | 19 +++++++++++++++
 arch/arm/boot/dts/sun8i-h3-nanopi-m1-plus.dts     | 29 +++++++++++++++++++++++
 arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts         |  7 ++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-2.dts         |  8 +++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-one.dts       |  8 +++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts   |  5 ++++
 arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts        |  8 +++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts      | 22 +++++++++++++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts    | 16 +++++++++++++
 10 files changed, 131 insertions(+)

--- a/arch/arm/boot/dts/sun8i-h2-plus-orangepi-zero.dts
+++ b/arch/arm/boot/dts/sun8i-h2-plus-orangepi-zero.dts
@@ -56,6 +56,8 @@
 
 	aliases {
 		serial0 = &uart0;
+		/* ethernet0 is the H3 emac, defined in sun8i-h3.dtsi */
+		ethernet0 = &emac;
 		ethernet1 = &xr819;
 	};
 
@@ -102,6 +104,13 @@
 	status = "okay";
 };
 
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>;
--- a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
@@ -52,6 +52,7 @@
 	compatible = "sinovoip,bpi-m2-plus", "allwinner,sun8i-h3";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 		serial1 = &uart1;
 	};
@@ -114,6 +115,24 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <0>;
+	};
+};
+
 &ir {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ir_pins_a>;
--- a/arch/arm/boot/dts/sun8i-h3-nanopi-m1-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-m1-plus.dts
@@ -45,6 +45,16 @@
 / {
 	model = "FriendlyArm NanoPi M1 Plus";
 	compatible = "friendlyarm,nanopi-m1-plus", "allwinner,sun8i-h3";
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+	};
 };
 
 &ehci1 {
@@ -55,6 +65,25 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	allwinner,leds-active-low;
+
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <7>;
+	};
+};
+
 &ohci1 {
 	status = "okay";
 };
--- a/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts
@@ -46,3 +46,10 @@
 	model = "FriendlyARM NanoPi NEO";
 	compatible = "friendlyarm,nanopi-neo", "allwinner,sun8i-h3";
 };
+
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts
@@ -54,6 +54,7 @@
 	aliases {
 		serial0 = &uart0;
 		/* ethernet0 is the H3 emac, defined in sun8i-h3.dtsi */
+		ethernet0 = &emac;
 		ethernet1 = &rtl8189;
 	};
 
@@ -117,6 +118,13 @@
 	status = "okay";
 };
 
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &ir {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ir_pins_a>;
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-one.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-one.dts
@@ -52,6 +52,7 @@
 	compatible = "xunlong,orangepi-one", "allwinner,sun8i-h3";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -97,6 +98,13 @@
 	status = "okay";
 };
 
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin>;
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts
@@ -53,6 +53,11 @@
 	};
 };
 
+&emac {
+	/* LEDs changed to active high on the plus */
+	/delete-property/ allwinner,leds-active-low;
+};
+
 &mmc1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc1_pins_a>;
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts
@@ -52,6 +52,7 @@
 	compatible = "xunlong,orangepi-pc", "allwinner,sun8i-h3";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -113,6 +114,13 @@
 	status = "okay";
 };
 
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &ir {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ir_pins_a>;
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts
@@ -47,6 +47,10 @@
 	model = "Xunlong Orange Pi Plus / Plus 2";
 	compatible = "xunlong,orangepi-plus", "allwinner,sun8i-h3";
 
+	aliases {
+		ethernet0 = &emac;
+	};
+
 	reg_gmac_3v3: gmac-3v3 {
 		compatible = "regulator-fixed";
 		regulator-name = "gmac-3v3";
@@ -74,6 +78,24 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <0>;
+	};
+};
+
 &mmc2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc2_8bit_pins>;
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts
@@ -61,3 +61,19 @@
 		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>; /* PD6 */
 	};
 };
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
