From: Vijay Viswanath <vviswana@codeaurora.org>
Date: Wed, 27 Sep 2017 11:04:42 +0530
Subject: [PATCH v2 3/4] mmc: Kconfig: Enable CONFIG_MMC_SDHCI_IO_ACCESSORS

Enable CONFIG_MMC_SDHCI_IO_ACCESSORS so that SDHC controller specific
register read and write APIs, if registered, can be used.

Signed-off-by: Vijay Viswanath <vviswana@codeaurora.org>
Acked-by: Adrian Hunter <adrian.hunter@intel.com>
---
 drivers/mmc/host/Kconfig | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mmc/host/Kconfig
+++ b/drivers/mmc/host/Kconfig
@@ -310,6 +310,7 @@ config MMC_SDHCI_BCM_KONA
 	tristate "SDHCI support on Broadcom KONA platform"
 	depends on ARCH_BCM_MOBILE
 	depends on MMC_SDHCI_PLTFM
+	select MMC_SDHCI_IO_ACCESSORS
 	help
 	  This selects the Broadcom Kona Secure Digital Host Controller
 	  Interface(SDHCI) support.
