From 11f8ad1656035176bad9d89de7ea0e7fe6d82c32 Mon Sep 17 00:00:00 2001
From: Stanislaw Gruszka <sgruszka@redhat.com>
Date: Sat, 9 Feb 2019 12:08:32 +0100
X-Patchwork-Submitter: Stanislaw Gruszka <sgruszka@redhat.com>
X-Patchwork-Id: 10804439
X-Patchwork-Delegate: kvalo@adurom.com
Subject: [PATCH 22/28] rt2800: new flush implementation for SoC devices

Use new flush_queue() calback for SoC devices, what was already done for
PCIe devices.

Signed-off-by: Stanislaw Gruszka <sgruszka@redhat.com>
---
 drivers/net/wireless/ralink/rt2x00/rt2800soc.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800soc.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800soc.c
@@ -203,7 +203,7 @@ static const struct rt2x00lib_ops rt2800
 	.start_queue		= rt2800mmio_start_queue,
 	.kick_queue		= rt2800mmio_kick_queue,
 	.stop_queue		= rt2800mmio_stop_queue,
-	.flush_queue		= rt2x00mmio_flush_queue,
+	.flush_queue		= rt2800mmio_flush_queue,
 	.write_tx_desc		= rt2800mmio_write_tx_desc,
 	.write_tx_data		= rt2800_write_tx_data,
 	.write_beacon		= rt2800_write_beacon,
