--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -9000,6 +9000,954 @@ restore_value:
 }
 EXPORT_SYMBOL_GPL(rt2800_rxiq_calibration);
 
+static void rt2800_rf_configstore(struct rt2x00_dev *rt2x00dev, rf_reg_pair rf_reg_record[][13], u8 chain)
+{
+	u8 rfvalue = 0;
+
+	if (chain == CHAIN_0) {
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 0, 1);
+		rf_reg_record[CHAIN_0][0].bank = 0;
+		rf_reg_record[CHAIN_0][0].reg = 1;
+		rf_reg_record[CHAIN_0][0].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 0, 2);
+		rf_reg_record[CHAIN_0][1].bank = 0;
+		rf_reg_record[CHAIN_0][1].reg = 2;
+		rf_reg_record[CHAIN_0][1].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 0, 35);
+		rf_reg_record[CHAIN_0][2].bank = 0;
+		rf_reg_record[CHAIN_0][2].reg = 35;
+		rf_reg_record[CHAIN_0][2].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 0, 42);
+		rf_reg_record[CHAIN_0][3].bank = 0;
+		rf_reg_record[CHAIN_0][3].reg = 42;
+		rf_reg_record[CHAIN_0][3].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 4, 0);
+		rf_reg_record[CHAIN_0][4].bank = 4;
+		rf_reg_record[CHAIN_0][4].reg = 0;
+		rf_reg_record[CHAIN_0][4].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 4, 2);
+		rf_reg_record[CHAIN_0][5].bank = 4;
+		rf_reg_record[CHAIN_0][5].reg = 2;
+		rf_reg_record[CHAIN_0][5].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 4, 34);
+		rf_reg_record[CHAIN_0][6].bank = 4;
+		rf_reg_record[CHAIN_0][6].reg = 34;
+		rf_reg_record[CHAIN_0][6].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 5, 3);
+		rf_reg_record[CHAIN_0][7].bank = 5;
+		rf_reg_record[CHAIN_0][7].reg = 3;
+		rf_reg_record[CHAIN_0][7].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 5, 4);
+		rf_reg_record[CHAIN_0][8].bank = 5;
+		rf_reg_record[CHAIN_0][8].reg = 4;
+		rf_reg_record[CHAIN_0][8].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 5, 17);
+		rf_reg_record[CHAIN_0][9].bank = 5;
+		rf_reg_record[CHAIN_0][9].reg = 17;
+		rf_reg_record[CHAIN_0][9].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 5, 18);
+		rf_reg_record[CHAIN_0][10].bank = 5;
+		rf_reg_record[CHAIN_0][10].reg = 18;
+		rf_reg_record[CHAIN_0][10].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 5, 19);
+		rf_reg_record[CHAIN_0][11].bank = 5;
+		rf_reg_record[CHAIN_0][11].reg = 19;
+		rf_reg_record[CHAIN_0][11].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 5, 20);
+		rf_reg_record[CHAIN_0][12].bank = 5;
+		rf_reg_record[CHAIN_0][12].reg = 20;
+		rf_reg_record[CHAIN_0][12].value = rfvalue;
+	} else if (chain == CHAIN_1) {
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 0, 1);
+		rf_reg_record[CHAIN_1][0].bank = 0;
+		rf_reg_record[CHAIN_1][0].reg = 1;
+		rf_reg_record[CHAIN_1][0].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 0, 2);
+		rf_reg_record[CHAIN_1][1].bank = 0;
+		rf_reg_record[CHAIN_1][1].reg = 2;
+		rf_reg_record[CHAIN_1][1].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 0, 35);
+		rf_reg_record[CHAIN_1][2].bank = 0;
+		rf_reg_record[CHAIN_1][2].reg = 35;
+		rf_reg_record[CHAIN_1][2].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 0, 42);
+		rf_reg_record[CHAIN_1][3].bank = 0;
+		rf_reg_record[CHAIN_1][3].reg = 42;
+		rf_reg_record[CHAIN_1][3].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 6, 0);
+		rf_reg_record[CHAIN_1][4].bank = 6;
+		rf_reg_record[CHAIN_1][4].reg = 0;
+		rf_reg_record[CHAIN_1][4].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 6, 2);
+		rf_reg_record[CHAIN_1][5].bank = 6;
+		rf_reg_record[CHAIN_1][5].reg = 2;
+		rf_reg_record[CHAIN_1][5].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 6, 34);
+		rf_reg_record[CHAIN_1][6].bank = 6;
+		rf_reg_record[CHAIN_1][6].reg = 34;
+		rf_reg_record[CHAIN_1][6].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 7, 3);
+		rf_reg_record[CHAIN_1][7].bank = 7;
+		rf_reg_record[CHAIN_1][7].reg = 3;
+		rf_reg_record[CHAIN_1][7].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 7, 4);
+		rf_reg_record[CHAIN_1][8].bank = 7;
+		rf_reg_record[CHAIN_1][8].reg = 4;
+		rf_reg_record[CHAIN_1][8].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 7, 17);
+		rf_reg_record[CHAIN_1][9].bank = 7;
+		rf_reg_record[CHAIN_1][9].reg = 17;
+		rf_reg_record[CHAIN_1][9].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 7, 18);
+		rf_reg_record[CHAIN_1][10].bank = 7;
+		rf_reg_record[CHAIN_1][10].reg = 18;
+		rf_reg_record[CHAIN_1][10].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 7, 19);
+		rf_reg_record[CHAIN_1][11].bank = 7;
+		rf_reg_record[CHAIN_1][11].reg = 19;
+		rf_reg_record[CHAIN_1][11].value = rfvalue;
+		rfvalue = rt2800_rfcsr_read_bank(rt2x00dev, 7, 20);
+		rf_reg_record[CHAIN_1][12].bank = 7;
+		rf_reg_record[CHAIN_1][12].reg = 20;
+		rf_reg_record[CHAIN_1][12].value = rfvalue;
+	} else {
+		rt2x00_warn(rt2x00dev, "Unknown chain = %u\n", chain);
+		return;
+	}
+
+	return;
+}
+EXPORT_SYMBOL_GPL(rt2800_rf_configstore);
+
+static void rt2800_rf_configrecover(struct rt2x00_dev *rt2x00dev, rf_reg_pair rf_record[][13])
+{
+	u8 chain_index = 0, record_index = 0;
+	u8 bank = 0, rf_register = 0, value = 0;
+
+	for (chain_index = 0; chain_index < 2; chain_index++) {
+		for (record_index = 0; record_index < 13; record_index++) {
+			bank = rf_record[chain_index][record_index].bank;
+			rf_register = rf_record[chain_index][record_index].reg;
+			value = rf_record[chain_index][record_index].value;
+			rt2800_rfcsr_write_bank(rt2x00dev, bank, rf_register, value);
+			rt2x00_dbg(rt2x00dev, "bank: %d, rf_register: %d, value: %x\n", bank, rf_register, value);
+		}
+	}
+
+	return;
+}
+EXPORT_SYMBOL_GPL(rt2800_rf_configrecover);
+
+static void rt2800_setbbptonegenerator(struct rt2x00_dev *rt2x00dev)
+{
+	rt2800_bbp_write(rt2x00dev, 158, 0xAA);
+	rt2800_bbp_write(rt2x00dev, 159, 0x00);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0xAB);
+	rt2800_bbp_write(rt2x00dev, 159, 0x0A);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0xAC);
+	rt2800_bbp_write(rt2x00dev, 159, 0x3F);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0xAD);
+	rt2800_bbp_write(rt2x00dev, 159, 0x3F);
+
+	rt2800_bbp_write(rt2x00dev, 244, 0x40);
+
+	return;
+}
+EXPORT_SYMBOL_GPL(rt2800_setbbptonegenerator);
+
+u32 rt2800_do_fft_accumulation(struct rt2x00_dev *rt2x00dev, u8 tidx, u8 read_neg)
+{
+	u32 macvalue = 0;
+	int fftout_i = 0, fftout_q = 0;
+	u32 ptmp=0, pint = 0;
+	u8 bbp = 0;
+	u8 tidxi;
+
+	rt2800_bbp_write(rt2x00dev, 158, 0x00);
+	rt2800_bbp_write(rt2x00dev, 159, 0x9b);
+
+	bbp = 0x9b;
+
+	while (bbp == 0x9b) {
+		udelay(10);
+		bbp = rt2800_bbp_read(rt2x00dev, 159);
+		bbp = bbp & 0xff;
+	}
+
+	rt2800_bbp_write(rt2x00dev, 158, 0xba);
+	rt2800_bbp_write(rt2x00dev, 159, tidx);
+	rt2800_bbp_write(rt2x00dev, 159, tidx);
+	rt2800_bbp_write(rt2x00dev, 159, tidx);
+
+	macvalue = rt2800_register_read(rt2x00dev, 0x057C);
+
+	fftout_i = (macvalue >> 16);
+	fftout_i = (fftout_i & 0x8000) ? (fftout_i - 0x10000) : fftout_i;
+	fftout_q = (macvalue & 0xffff);
+	fftout_q = (fftout_q & 0x8000) ? (fftout_q - 0x10000) : fftout_q;
+	ptmp = (fftout_i * fftout_i);
+	ptmp = ptmp + (fftout_q * fftout_q);
+	pint = ptmp;
+	rt2x00_dbg(rt2x00dev, "I = %d,  Q = %d, power = %x\n", fftout_i, fftout_q, pint);
+	if (read_neg) {
+		pint = pint >> 1;
+		tidxi = 0x40 - tidx;
+		tidxi = tidxi & 0x3f;
+
+		rt2800_bbp_write(rt2x00dev, 158, 0xba);
+		rt2800_bbp_write(rt2x00dev, 159, tidxi);
+		rt2800_bbp_write(rt2x00dev, 159, tidxi);
+		rt2800_bbp_write(rt2x00dev, 159, tidxi);
+
+		macvalue = rt2800_register_read(rt2x00dev, 0x057C);
+
+		fftout_i = (macvalue >> 16);
+		fftout_i = (fftout_i & 0x8000) ? (fftout_i - 0x10000) : fftout_i;
+		fftout_q = (macvalue & 0xffff);
+		fftout_q = (fftout_q & 0x8000) ? (fftout_q - 0x10000) : fftout_q;
+		ptmp = (fftout_i * fftout_i);
+		ptmp = ptmp + (fftout_q * fftout_q);
+		ptmp = ptmp >> 1;
+		pint = pint + ptmp;
+	}
+
+	return pint;
+}
+EXPORT_SYMBOL_GPL(rt2800_do_fft_accumulation);
+
+u32 rt2800_read_fft_accumulation(struct rt2x00_dev *rt2x00dev, u8 tidx) {
+	u32 macvalue = 0;
+	int fftout_i = 0, fftout_q = 0;
+	u32 ptmp=0, pint = 0;
+
+	rt2800_bbp_write(rt2x00dev, 158, 0xBA);
+	rt2800_bbp_write(rt2x00dev, 159, tidx);
+	rt2800_bbp_write(rt2x00dev, 159, tidx);
+	rt2800_bbp_write(rt2x00dev, 159, tidx);
+
+	macvalue = rt2800_register_read(rt2x00dev, 0x057C);
+
+	fftout_i = (macvalue >> 16);
+	fftout_i = (fftout_i & 0x8000) ? (fftout_i - 0x10000) : fftout_i;
+	fftout_q = (macvalue & 0xffff);
+	fftout_q = (fftout_q & 0x8000) ? (fftout_q - 0x10000) : fftout_q;
+	ptmp = (fftout_i * fftout_i);
+	ptmp = ptmp + (fftout_q * fftout_q);
+	pint = ptmp;
+	rt2x00_info(rt2x00dev, "I = %d,  Q = %d, power = %x\n", fftout_i, fftout_q, pint);
+
+	return pint;
+}
+EXPORT_SYMBOL_GPL(rt2800_read_fft_accumulation);
+
+static void rt2800_write_dc(struct rt2x00_dev *rt2x00dev, u8 ch_idx, u8 alc, u8 iorq, u8 dc)
+{
+	u8 bbp = 0;
+
+	rt2800_bbp_write(rt2x00dev, 158, 0xb0);
+	bbp = alc | 0x80;
+	rt2800_bbp_write(rt2x00dev, 159, bbp);
+
+	if (ch_idx == 0)
+		bbp = (iorq == 0) ? 0xb1: 0xb2;
+	else
+		bbp = (iorq == 0) ? 0xb8: 0xb9;
+
+	rt2800_bbp_write(rt2x00dev, 158, bbp);
+	bbp = dc;
+	rt2800_bbp_write(rt2x00dev, 159, bbp);
+
+	return;
+}
+EXPORT_SYMBOL_GPL(rt2800_write_dc);
+
+static void rt2800_loft_search(struct rt2x00_dev *rt2x00dev, u8 ch_idx, u8 alc_idx, u8 dc_result[][RF_ALC_NUM][2])
+{
+	u32 p0 = 0, p1 = 0, pf = 0;
+	char idx0 = 0, idx1 = 0;
+	u8 idxf[] = {0x00, 0x00};
+	u8 ibit = 0x20;
+	u8 iorq;
+	char bidx;
+
+	rt2800_bbp_write(rt2x00dev, 158, 0xb0);
+	rt2800_bbp_write(rt2x00dev, 159, 0x80);
+
+	for (bidx = 5; bidx >= 0; bidx--) {
+		for (iorq = 0; iorq <= 1; iorq++) {
+			rt2x00_dbg(rt2x00dev, "\n========================================================\n");
+
+			if (idxf[iorq] == 0x20) {
+				idx0 = 0x20;
+				p0 = pf;
+			} else {
+				idx0 = idxf[iorq] - ibit;
+				idx0 = idx0 & 0x3F;
+				rt2800_write_dc(rt2x00dev, ch_idx, 0, iorq, idx0);
+				p0 = rt2800_do_fft_accumulation(rt2x00dev, 0x0A, 0);
+			}
+
+			idx1 = idxf[iorq] + ((bidx == 5) ? 0 : ibit);
+			idx1 = idx1 & 0x3F;
+			rt2800_write_dc(rt2x00dev, ch_idx, 0, iorq, idx1);
+			p1 = rt2800_do_fft_accumulation(rt2x00dev, 0x0A, 0);
+
+			rt2x00_dbg(rt2x00dev, "alc=%u, IorQ=%u, idx_final=%2x\n", alc_idx, iorq, idxf[iorq]);
+			rt2x00_dbg(rt2x00dev, "p0=%x, p1=%x, pf=%x, idx_0=%x, idx_1=%x, ibit=%x !\n", p0, p1, pf, idx0, idx1, ibit);
+
+			if ((bidx != 5) && (pf <= p0) && (pf < p1)) {
+				pf = pf;
+				idxf[iorq] = idxf[iorq];
+			} else if (p0 < p1) {
+				pf = p0;
+				idxf[iorq] = idx0 & 0x3F;
+			} else {
+				pf = p1;
+				idxf[iorq] = idx1 & 0x3F;
+			}
+			rt2x00_dbg(rt2x00dev, "IorQ=%u, idx_final[%u]:%x, pf:%8x\n", iorq, iorq, idxf[iorq], pf);
+
+			rt2800_write_dc(rt2x00dev, ch_idx, 0, iorq, idxf[iorq]);
+
+		}
+		ibit = ibit >> 1;
+	}
+	dc_result[ch_idx][alc_idx][0] = idxf[0];
+	dc_result[ch_idx][alc_idx][1] = idxf[1];
+
+	return;
+}
+EXPORT_SYMBOL_GPL(rt2800_loft_search);
+
+static void rt2800_iq_search(struct rt2x00_dev *rt2x00dev, u8 ch_idx, u8 *ges, u8 *pes)
+{
+	u32 p0 = 0, p1 = 0, pf = 0;
+	char perr = 0, gerr = 0, iq_err = 0;
+	char pef = 0, gef = 0;
+	char psta, pend;
+	char gsta, gend;
+
+	u8 ibit = 0x20;
+	u8 first_search = 0x00, touch_neg_max = 0x00;
+	char idx0 = 0, idx1 = 0;
+	u8 gop;
+	u8 bbp = 0;
+	char bidx;
+
+	rt2x00_info(rt2x00dev, "IQCalibration Start!\n");
+	for (bidx = 5; bidx >= 1; bidx--) {
+		for (gop = 0; gop < 2; gop++) {
+			rt2x00_dbg(rt2x00dev, "\n========================================================\n");
+
+			if ((gop == 1) || (bidx < 4)) {
+				if (gop == 0)
+					iq_err = gerr;
+				else
+					iq_err = perr;
+
+				first_search = (gop == 0) ? (bidx == 3) : (bidx == 5);
+				touch_neg_max = (gop) ? ((iq_err & 0x0F) == 0x08) : ((iq_err & 0x3F) == 0x20);
+
+				if (touch_neg_max) {
+					p0 = pf;
+					idx0 = iq_err;
+				} else {
+					idx0 = iq_err - ibit;
+					bbp = (ch_idx == 0) ? ((gop == 0) ? 0x28 : 0x29): ((gop == 0) ? 0x46 : 0x47);
+
+					rt2800_bbp_write(rt2x00dev, 158, bbp);
+					rt2800_bbp_write(rt2x00dev, 159, idx0);
+
+					p0 = rt2800_do_fft_accumulation(rt2x00dev, 0x14, 1);
+				}
+
+				idx1 = iq_err + (first_search ? 0 : ibit);
+				idx1 = (gop == 0) ? (idx1 & 0x0F) : (idx1 & 0x3F);
+
+				bbp = (ch_idx == 0) ? (gop == 0) ? 0x28 : 0x29 : (gop == 0) ? 0x46 : 0x47;
+
+				rt2800_bbp_write(rt2x00dev, 158, bbp);
+				rt2800_bbp_write(rt2x00dev, 159, idx1);
+
+				p1 = rt2800_do_fft_accumulation(rt2x00dev, 0x14, 1);
+
+				rt2x00_dbg(rt2x00dev, "p0=%x, p1=%x, pwer_final=%x, idx0=%x, idx1=%x, iq_err=%x, gop=%d, ibit=%x !\n", p0, p1, pf, idx0, idx1, iq_err, gop, ibit);
+
+				if ((!first_search) && (pf <= p0) && (pf < p1)) {
+					pf = pf;
+				} else if (p0 < p1) {
+					pf = p0;
+					iq_err = idx0;
+				} else {
+					pf = p1;
+					iq_err = idx1;
+				}
+
+				bbp = (ch_idx == 0) ? (gop == 0) ? 0x28 : 0x29 : (gop == 0) ? 0x46 : 0x47;
+
+				rt2800_bbp_write(rt2x00dev, 158, bbp);
+				rt2800_bbp_write(rt2x00dev, 159, iq_err);
+
+				if (gop == 0)
+					gerr = iq_err;
+				else
+					perr = iq_err;
+
+				rt2x00_dbg(rt2x00dev, "IQCalibration pf=%8x (%2x, %2x) !\n", pf, gerr & 0x0F, perr & 0x3F);
+
+			}
+		}
+
+		if (bidx > 0)
+			ibit = (ibit >> 1);
+	}
+	gerr = (gerr & 0x08) ? (gerr & 0x0F) - 0x10 : (gerr & 0x0F);
+	perr = (perr & 0x20) ? (perr & 0x3F) - 0x40 : (perr & 0x3F);
+
+	gerr = (gerr < -0x07) ? -0x07 : (gerr > 0x05) ? 0x05 : gerr;
+	gsta = gerr - 1;
+	gend = gerr + 2;
+
+	perr = (perr < -0x1f) ? -0x1f : (perr > 0x1d) ? 0x1d : perr;
+	psta = perr - 1;
+	pend = perr + 2;
+
+	for (gef = gsta; gef <= gend; gef = gef + 1)
+		for (pef = psta; pef <= pend; pef = pef + 1) {
+			bbp = (ch_idx == 0) ? 0x28 : 0x46;
+			rt2800_bbp_write(rt2x00dev, 158, bbp);
+			rt2800_bbp_write(rt2x00dev, 159, gef & 0x0F);
+
+			bbp = (ch_idx == 0) ? 0x29 : 0x47;
+			rt2800_bbp_write(rt2x00dev, 158, bbp);
+			rt2800_bbp_write(rt2x00dev, 159, pef & 0x3F);
+
+			p1 = rt2800_do_fft_accumulation(rt2x00dev, 0x14, 1);
+			if ((gef == gsta) && (pef == psta)) {
+				pf = p1;
+				gerr = gef;
+				perr = pef;
+			}
+			else if (pf > p1){
+				pf = p1;
+				gerr = gef;
+				perr = pef;
+			}
+			rt2x00_dbg(rt2x00dev, "Fine IQCalibration p1=%8x pf=%8x (%2x, %2x) !\n", p1, pf, gef & 0x0F, pef & 0x3F);
+		}
+
+	ges[ch_idx] = gerr & 0x0F;
+	pes[ch_idx] = perr & 0x3F;
+
+	rt2x00_info(rt2x00dev, "IQCalibration Done! CH = %u, (gain=%2x, phase=%2x)\n", ch_idx, gerr & 0x0F, perr & 0x3F);
+
+	return;
+}
+EXPORT_SYMBOL_GPL(rt2800_iq_search);
+
+static void rt2800_rf_aux_tx0_loopback(struct rt2x00_dev *rt2x00dev)
+{
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 1, 0x21);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 2, 0x10);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 35, 0x00);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 42, 0x1b);
+	rt2800_rfcsr_write_bank(rt2x00dev, 4, 0, 0x81);
+	rt2800_rfcsr_write_bank(rt2x00dev, 4, 2, 0x81);
+	rt2800_rfcsr_write_bank(rt2x00dev, 4, 34, 0xee);
+	rt2800_rfcsr_write_bank(rt2x00dev, 5, 3, 0x2d);
+	rt2800_rfcsr_write_bank(rt2x00dev, 5, 4, 0x2d);
+	rt2800_rfcsr_write_bank(rt2x00dev, 5, 17, 0x80);
+	rt2800_rfcsr_write_bank(rt2x00dev, 5, 18, 0xd7);
+	rt2800_rfcsr_write_bank(rt2x00dev, 5, 19, 0xa2);
+	rt2800_rfcsr_write_bank(rt2x00dev, 5, 20, 0x20);
+}
+EXPORT_SYMBOL_GPL(rt2800_rf_aux_tx0_loopback);
+
+static void rt2800_rf_aux_tx1_loopback(struct rt2x00_dev *rt2x00dev)
+{
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 1, 0x22);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 2, 0x20);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 35, 0x00);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 42, 0x4b);
+	rt2800_rfcsr_write_bank(rt2x00dev, 6, 0, 0x81);
+	rt2800_rfcsr_write_bank(rt2x00dev, 6, 2, 0x81);
+	rt2800_rfcsr_write_bank(rt2x00dev, 6, 34, 0xee);
+	rt2800_rfcsr_write_bank(rt2x00dev, 7, 3, 0x2d);
+	rt2800_rfcsr_write_bank(rt2x00dev, 7, 4, 0x2d);
+	rt2800_rfcsr_write_bank(rt2x00dev, 7, 17, 0x80);
+	rt2800_rfcsr_write_bank(rt2x00dev, 7, 18, 0xd7);
+	rt2800_rfcsr_write_bank(rt2x00dev, 7, 19, 0xa2);
+	rt2800_rfcsr_write_bank(rt2x00dev, 7, 20, 0x20);
+}
+EXPORT_SYMBOL_GPL(rt2800_rf_aux_tx1_loopback);
+
+void rt2800_loft_iq_calibration(struct rt2x00_dev *rt2x00dev)
+{
+	rf_reg_pair rf_store[CHAIN_NUM][13];
+	u32 macorg1 = 0;
+	u32 macorg2 = 0;
+	u32 macorg3 = 0;
+	u32 macorg4 = 0;
+	u32 macorg5 = 0;
+	u32 orig528 = 0;
+	u32 orig52c = 0;
+
+	u32 savemacsysctrl = 0, mtxcycle = 0;
+	u32 macvalue = 0;
+	u32 mac13b8 = 0;
+	u32 p0 = 0, p1 = 0;
+	u32 p0_idx10 = 0, p1_idx10 = 0;
+
+	u8 rfvalue;
+	u8 loft_dc_search_result[CHAIN_NUM][RF_ALC_NUM][2];
+	u8 ger[CHAIN_NUM], per[CHAIN_NUM];
+	u8 rf_gain[] = {0x00, 0x01, 0x02, 0x04, 0x08, 0x0c};
+	u8 rfvga_gain_table[] = {0x24, 0x25, 0x26, 0x27, 0x28, 0x2c, 0x2d, 0x2e, 0x2f, 0x30, 0x31, 0x38, 0x39, 0x3a, 0x3b, 0x3c, 0x3d, 0x3e, 0x3F};
+
+	u8 vga_gain[] = {14, 14};
+	u8 bbp_2324gain[] = {0x16, 0x14, 0x12, 0x10, 0x0c, 0x08};
+	u8 bbp = 0, ch_idx = 0, rf_alc_idx = 0, idx = 0;
+	u8 bbpr30, rfb0r39, rfb0r42;
+	u8 bbpr1;
+	u8 bbpr4;
+	u8 bbpr241, bbpr242;
+	u8 count_step;
+
+	savemacsysctrl = rt2800_register_read(rt2x00dev, MAC_SYS_CTRL);
+	macorg1 = rt2800_register_read(rt2x00dev, TX_PIN_CFG);
+	macorg2 = rt2800_register_read(rt2x00dev, RF_CONTROL0);
+	macorg3 = rt2800_register_read(rt2x00dev, RF_BYPASS0);
+	macorg4 = rt2800_register_read(rt2x00dev, RF_CONTROL3);
+	macorg5 = rt2800_register_read(rt2x00dev, RF_BYPASS3);
+	mac13b8 = rt2800_register_read(rt2x00dev, 0x13b8);
+	orig528 = rt2800_register_read(rt2x00dev, RF_CONTROL2);
+	orig52c = rt2800_register_read(rt2x00dev, RF_BYPASS2);
+
+	macvalue = rt2800_register_read(rt2x00dev, MAC_SYS_CTRL);
+	macvalue &= (~0x04);
+	rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, macvalue);
+
+	for (mtxcycle = 0; mtxcycle < 10000; mtxcycle++) {
+		macvalue = rt2800_register_read(rt2x00dev, MAC_STATUS_CFG);
+		if (macvalue & 0x01)
+			udelay(50);
+		else
+			break;
+	}
+
+	macvalue = rt2800_register_read(rt2x00dev, MAC_SYS_CTRL);
+	macvalue &= (~0x08);
+	rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, macvalue);
+
+	for (mtxcycle = 0; mtxcycle < 10000; mtxcycle++) {
+		macvalue = rt2800_register_read(rt2x00dev, MAC_STATUS_CFG);
+		if (macvalue & 0x02)
+			udelay(50);
+		else
+			break;
+	}
+
+	for (ch_idx = 0; ch_idx < 2; ch_idx++) {
+		rt2800_rf_configstore(rt2x00dev, rf_store, ch_idx);
+	}
+
+	bbpr30 = rt2800_bbp_read(rt2x00dev, 30);
+	rfb0r39 = rt2800_rfcsr_read_bank(rt2x00dev, 0, 39);
+	rfb0r42 = rt2800_rfcsr_read_bank(rt2x00dev, 0, 42);
+
+	rt2800_bbp_write(rt2x00dev, 30, 0x1F);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 39, 0x80);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 42, 0x5B);
+
+	rt2800_bbp_write(rt2x00dev, 23, 0x00);
+	rt2800_bbp_write(rt2x00dev, 24, 0x00);
+
+	rt2800_setbbptonegenerator(rt2x00dev);
+
+	for (ch_idx = 0; ch_idx < 2; ch_idx ++) {
+		rt2800_bbp_write(rt2x00dev, 23, 0x00);
+		rt2800_bbp_write(rt2x00dev, 24, 0x00);
+		rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, 0x00);
+		rt2800_register_write(rt2x00dev, TX_PIN_CFG, 0x0000000F);
+		rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x00000004);
+		rt2800_register_write(rt2x00dev, RF_BYPASS0, 0x00003306);
+		rt2800_register_write(rt2x00dev, 0x13b8, 0x10);
+		udelay(1);
+
+		if (ch_idx == 0) {
+			rt2800_rf_aux_tx0_loopback(rt2x00dev);
+		} else {
+			rt2800_rf_aux_tx1_loopback(rt2x00dev);
+		}
+		udelay(1);
+
+		if (ch_idx == 0) {
+			rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x00001004);
+		} else {
+			rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x00002004);
+		}
+
+		rt2800_bbp_write(rt2x00dev, 158, 0x05);
+		rt2800_bbp_write(rt2x00dev, 159, 0x00);
+
+		rt2800_bbp_write(rt2x00dev, 158, 0x01);
+		if (ch_idx == 0)
+			rt2800_bbp_write(rt2x00dev, 159, 0x00);
+		else
+			rt2800_bbp_write(rt2x00dev, 159, 0x01);
+
+		vga_gain[ch_idx] = 18;
+		for (rf_alc_idx = 0; rf_alc_idx < 3; rf_alc_idx++) {
+			rt2800_bbp_write(rt2x00dev, 23, bbp_2324gain[rf_alc_idx]);
+			rt2800_bbp_write(rt2x00dev, 24, bbp_2324gain[rf_alc_idx]);
+
+			macvalue = rt2800_register_read(rt2x00dev, RF_CONTROL3);
+			macvalue &= (~0x0000F1F1);
+			macvalue |= (rf_gain[rf_alc_idx] << 4);
+			macvalue |= (rf_gain[rf_alc_idx] << 12);
+			rt2800_register_write(rt2x00dev, RF_CONTROL3, macvalue);
+			macvalue = (0x0000F1F1);
+			rt2800_register_write(rt2x00dev, RF_BYPASS3, macvalue);
+
+			if (rf_alc_idx == 0) {
+				rt2800_write_dc(rt2x00dev, ch_idx, 0, 1, 0x21);
+				for (;vga_gain[ch_idx] > 0;vga_gain[ch_idx] = vga_gain[ch_idx] - 2) {
+					rfvalue = rfvga_gain_table[vga_gain[ch_idx]];
+					rt2800_rfcsr_write_dccal(rt2x00dev, 3, rfvalue);
+					rt2800_rfcsr_write_dccal(rt2x00dev, 4, rfvalue);
+					rt2800_write_dc(rt2x00dev, ch_idx, 0, 1, 0x00);
+					rt2800_write_dc(rt2x00dev, ch_idx, 0, 0, 0x00);
+					p0 = rt2800_do_fft_accumulation(rt2x00dev, 0x0A, 0);
+					rt2800_write_dc(rt2x00dev, ch_idx, 0, 0, 0x21);
+					p1 = rt2800_do_fft_accumulation(rt2x00dev, 0x0A, 0);
+					rt2x00_dbg(rt2x00dev, "LOFT AGC %d %d\n", p0, p1);
+					if ((p0 < 7000*7000) && (p1 < (7000*7000))) {
+						break;
+					}
+				}
+
+				rt2800_write_dc(rt2x00dev, ch_idx, 0, 0, 0x00);
+				rt2800_write_dc(rt2x00dev, ch_idx, 0, 1, 0x00);
+
+				rt2x00_dbg(rt2x00dev, "Used VGA %d %x\n",vga_gain[ch_idx], rfvga_gain_table[vga_gain[ch_idx]]);
+
+				if (vga_gain[ch_idx] < 0)
+					vga_gain[ch_idx] = 0;
+		 	}
+
+			rfvalue = rfvga_gain_table[vga_gain[ch_idx]];
+
+			rt2800_rfcsr_write_dccal(rt2x00dev, 3, rfvalue);
+			rt2800_rfcsr_write_dccal(rt2x00dev, 4, rfvalue);
+
+			rt2800_loft_search(rt2x00dev, ch_idx, rf_alc_idx, loft_dc_search_result);
+		}
+	}
+
+	for (rf_alc_idx = 0; rf_alc_idx < 3; rf_alc_idx++) {
+		for (idx = 0; idx < 4; idx++) {
+			rt2800_bbp_write(rt2x00dev, 158, 0xB0);
+			bbp = (idx<<2) + rf_alc_idx;
+			rt2800_bbp_write(rt2x00dev, 159, bbp);
+			rt2x00_dbg(rt2x00dev, " ALC %2x,", bbp);
+
+			rt2800_bbp_write(rt2x00dev, 158, 0xb1);
+			bbp = loft_dc_search_result[CHAIN_0][rf_alc_idx][0x00];
+			bbp = bbp & 0x3F;
+			rt2800_bbp_write(rt2x00dev, 159, bbp);
+			rt2x00_dbg(rt2x00dev, " I0 %2x,", bbp);
+
+			rt2800_bbp_write(rt2x00dev, 158, 0xb2);
+			bbp = loft_dc_search_result[CHAIN_0][rf_alc_idx][0x01];
+			bbp = bbp & 0x3F;
+			rt2800_bbp_write(rt2x00dev, 159, bbp);
+			rt2x00_dbg(rt2x00dev, " Q0 %2x,", bbp);
+
+			rt2800_bbp_write(rt2x00dev, 158, 0xb8);
+			bbp = loft_dc_search_result[CHAIN_1][rf_alc_idx][0x00];
+			bbp = bbp & 0x3F;
+			rt2800_bbp_write(rt2x00dev, 159, bbp);
+			rt2x00_dbg(rt2x00dev, " I1 %2x,", bbp);
+
+			rt2800_bbp_write(rt2x00dev, 158, 0xb9);
+			bbp = loft_dc_search_result[CHAIN_1][rf_alc_idx][0x01];
+			bbp = bbp & 0x3F;
+			rt2800_bbp_write(rt2x00dev, 159, bbp);
+			rt2x00_dbg(rt2x00dev, " Q1 %2x\n", bbp);
+		}
+	}
+
+	rt2800_bbp_write(rt2x00dev, 23, 0x00);
+	rt2800_bbp_write(rt2x00dev, 24, 0x00);
+
+	rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x04);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0x00);
+	rt2800_bbp_write(rt2x00dev, 159, 0x00);
+
+	bbp = 0x00;
+	rt2800_bbp_write(rt2x00dev, 244, 0x00);
+
+	rt2800_bbp_write(rt2x00dev, 21, 0x01);
+	udelay(1);
+	rt2800_bbp_write(rt2x00dev, 21, 0x00);
+
+	rt2800_rf_configrecover(rt2x00dev, rf_store);
+
+	rt2800_register_write(rt2x00dev, TX_PIN_CFG, macorg1);
+	rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x04);
+	rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x00);
+	rt2800_register_write(rt2x00dev, RF_BYPASS0, 0x00);
+	rt2800_register_write(rt2x00dev, RF_CONTROL0, macorg2);
+	udelay(1);
+	rt2800_register_write(rt2x00dev, RF_BYPASS0, macorg3);
+	rt2800_register_write(rt2x00dev, RF_CONTROL3, macorg4);
+	rt2800_register_write(rt2x00dev, RF_BYPASS3, macorg5);
+	rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, savemacsysctrl);
+	rt2800_register_write(rt2x00dev, RF_CONTROL2, orig528);
+	rt2800_register_write(rt2x00dev, RF_BYPASS2, orig52c);
+	rt2800_register_write(rt2x00dev, 0x13b8, mac13b8);
+
+	rt2x00_info(rt2x00dev, "LOFT Calibration Done!\n");
+
+	savemacsysctrl = rt2800_register_read(rt2x00dev, MAC_SYS_CTRL);
+	macorg1 = rt2800_register_read(rt2x00dev, TX_PIN_CFG);
+	macorg2 = rt2800_register_read(rt2x00dev, RF_CONTROL0);
+	macorg3 = rt2800_register_read(rt2x00dev, RF_BYPASS0);
+	macorg4 = rt2800_register_read(rt2x00dev, RF_CONTROL3);
+	macorg5 = rt2800_register_read(rt2x00dev, RF_BYPASS3);
+
+	bbpr1 = rt2800_bbp_read(rt2x00dev, 1);
+	bbpr4 = rt2800_bbp_read(rt2x00dev, 4);
+	bbpr241 = rt2800_bbp_read(rt2x00dev, 241);
+	bbpr242 = rt2800_bbp_read(rt2x00dev, 242);
+	mac13b8 = rt2800_register_read(rt2x00dev, 0x13b8);
+
+	macvalue = rt2800_register_read(rt2x00dev, MAC_SYS_CTRL);
+	macvalue &= (~0x04);
+	rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, macvalue);
+	for (mtxcycle = 0; mtxcycle < 10000; mtxcycle++) {
+		macvalue = rt2800_register_read(rt2x00dev, MAC_STATUS_CFG);
+		if (macvalue & 0x01)
+			udelay(50);
+		else
+			break;
+	}
+
+	macvalue = rt2800_register_read(rt2x00dev, MAC_SYS_CTRL);
+	macvalue &= (~0x08);
+	rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, macvalue);
+	for (mtxcycle = 0; mtxcycle < 10000; mtxcycle++) {
+		macvalue = rt2800_register_read(rt2x00dev, MAC_STATUS_CFG);
+		if (macvalue & 0x02)
+			udelay(50);
+		else
+			break;
+	}
+
+	if (test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+		rt2800_register_write(rt2x00dev, RF_CONTROL3, 0x00000101);
+		rt2800_register_write(rt2x00dev, RF_BYPASS3, 0x0000F1F1);
+	}
+
+	rt2800_bbp_write(rt2x00dev, 23, 0x00);
+	rt2800_bbp_write(rt2x00dev, 24, 0x00);
+
+	if (test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+		rt2800_bbp_write(rt2x00dev, 4, bbpr4 & (~0x18));
+		rt2800_bbp_write(rt2x00dev, 21, 0x01);
+		udelay(1);
+		rt2800_bbp_write(rt2x00dev, 21, 0x00);
+
+		rt2800_bbp_write(rt2x00dev, 241, 0x14);
+		rt2800_bbp_write(rt2x00dev, 242, 0x80);
+		rt2800_bbp_write(rt2x00dev, 244, 0x31);
+	} else {
+		rt2800_setbbptonegenerator(rt2x00dev);
+	}
+
+	rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x00000004);
+	rt2800_register_write(rt2x00dev, RF_BYPASS0, 0x00003306);
+	udelay(1);
+
+	rt2800_register_write(rt2x00dev, TX_PIN_CFG, 0x0000000F);
+
+	if (!test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+		rt2800_register_write(rt2x00dev, RF_CONTROL3, 0x00000000);
+		rt2800_register_write(rt2x00dev, RF_BYPASS3, 0x0000F1F1);
+	}
+
+	rt2800_register_write(rt2x00dev, 0x13b8, 0x00000010);
+
+	for (ch_idx = 0; ch_idx < 2; ch_idx++) {
+		rt2800_rf_configstore(rt2x00dev, rf_store, ch_idx);
+	}
+
+	rt2800_rfcsr_write_dccal(rt2x00dev, 3, 0x3B);
+	rt2800_rfcsr_write_dccal(rt2x00dev, 4, 0x3B);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0x03);
+	rt2800_bbp_write(rt2x00dev, 159, 0x60);
+	rt2800_bbp_write(rt2x00dev, 158, 0xB0);
+	rt2800_bbp_write(rt2x00dev, 159, 0x80);
+
+	for (ch_idx = 0; ch_idx < 2; ch_idx ++) {
+		rt2800_bbp_write(rt2x00dev, 23, 0x00);
+		rt2800_bbp_write(rt2x00dev, 24, 0x00);
+
+		if (ch_idx == 0) {
+			rt2800_bbp_write(rt2x00dev, 158, 0x01);
+			rt2800_bbp_write(rt2x00dev, 159, 0x00);
+			if (test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+				bbp = bbpr1 & (~0x18);
+				bbp = bbp | 0x00;
+				rt2800_bbp_write(rt2x00dev, 1, bbp);
+			}
+			rt2800_rf_aux_tx0_loopback(rt2x00dev);
+			rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x00001004);
+		} else {
+			rt2800_bbp_write(rt2x00dev, 158, 0x01);
+			rt2800_bbp_write(rt2x00dev, 159, 0x01);
+			if (test_bit(CAPABILITY_EXTERNAL_PA_TX1, &rt2x00dev->cap_flags)) {
+				bbp = bbpr1 & (~0x18);
+				bbp = bbp | 0x08;
+				rt2800_bbp_write(rt2x00dev, 1, bbp);
+			}
+			rt2800_rf_aux_tx1_loopback(rt2x00dev);
+			rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x00002004);
+		}
+
+		rt2800_bbp_write(rt2x00dev, 158, 0x05);
+		rt2800_bbp_write(rt2x00dev, 159, 0x04);
+
+		bbp = (ch_idx == 0) ? 0x28 : 0x46;
+		rt2800_bbp_write(rt2x00dev, 158, bbp);
+		rt2800_bbp_write(rt2x00dev, 159, 0x00);
+
+		if (test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+			rt2800_bbp_write(rt2x00dev, 23, 0x06);
+			rt2800_bbp_write(rt2x00dev, 24, 0x06);
+			count_step = 1;
+		} else {
+			rt2800_bbp_write(rt2x00dev, 23, 0x1F);
+			rt2800_bbp_write(rt2x00dev, 24, 0x1F);
+			count_step = 2;
+		}
+
+		for (;vga_gain[ch_idx] < 19; vga_gain[ch_idx]=(vga_gain[ch_idx] + count_step)) {
+			rfvalue = rfvga_gain_table[vga_gain[ch_idx]];
+			rt2800_rfcsr_write_dccal(rt2x00dev, 3, rfvalue);
+			rt2800_rfcsr_write_dccal(rt2x00dev, 4, rfvalue);
+
+			bbp = (ch_idx == 0) ? 0x29 : 0x47;
+			rt2800_bbp_write(rt2x00dev, 158, bbp);
+			rt2800_bbp_write(rt2x00dev, 159, 0x00);
+			p0 = rt2800_do_fft_accumulation(rt2x00dev, 0x14, 0);
+			if (test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+				p0_idx10 = rt2800_read_fft_accumulation(rt2x00dev, 0x0A);
+			}
+
+			bbp = (ch_idx == 0) ? 0x29 : 0x47;
+			rt2800_bbp_write(rt2x00dev, 158, bbp);
+			rt2800_bbp_write(rt2x00dev, 159, 0x21);
+			p1 = rt2800_do_fft_accumulation(rt2x00dev, 0x14, 0);
+			if (test_bit(CAPABILITY_EXTERNAL_PA_TX1, &rt2x00dev->cap_flags)) {
+				p1_idx10 = rt2800_read_fft_accumulation(rt2x00dev, 0x0A);
+			}
+
+			rt2x00_dbg(rt2x00dev, "IQ AGC %d %d\n", p0, p1);
+
+			if (test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+				rt2x00_dbg(rt2x00dev, "IQ AGC IDX 10 %d %d\n", p0_idx10, p1_idx10);
+				if ((p0_idx10 > 7000*7000) || (p1_idx10 > 7000*7000)) {
+					if (vga_gain[ch_idx]!=0)
+						vga_gain[ch_idx] = vga_gain[ch_idx]-1;
+					break;
+				}
+			}
+
+			if ((p0 > 2500*2500) || (p1 > 2500*2500)) {
+				break;
+			}
+		}
+
+		if (vga_gain[ch_idx] > 18)
+			vga_gain[ch_idx] = 18;
+		rt2x00_dbg(rt2x00dev, "Used VGA %d %x\n",vga_gain[ch_idx], rfvga_gain_table[vga_gain[ch_idx]]);
+
+		bbp = (ch_idx == 0) ? 0x29 : 0x47;
+		rt2800_bbp_write(rt2x00dev, 158, bbp);
+		rt2800_bbp_write(rt2x00dev, 159, 0x00);
+
+		rt2800_iq_search(rt2x00dev, ch_idx, ger, per);
+	}
+
+	rt2800_bbp_write(rt2x00dev, 23, 0x00);
+	rt2800_bbp_write(rt2x00dev, 24, 0x00);
+	rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x04);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0x28);
+	bbp = ger[CHAIN_0] & 0x0F;
+	rt2800_bbp_write(rt2x00dev, 159, bbp);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0x29);
+	bbp = per[CHAIN_0] & 0x3F;
+	rt2800_bbp_write(rt2x00dev, 159, bbp);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0x46);
+	bbp = ger[CHAIN_1] & 0x0F;
+	rt2800_bbp_write(rt2x00dev, 159, bbp);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0x47);
+	bbp = per[CHAIN_1] & 0x3F;
+	rt2800_bbp_write(rt2x00dev, 159, bbp);
+
+	if (test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+		rt2800_bbp_write(rt2x00dev, 1, bbpr1);
+		rt2800_bbp_write(rt2x00dev, 241, bbpr241);
+		rt2800_bbp_write(rt2x00dev, 242, bbpr242);
+	}
+	rt2800_bbp_write(rt2x00dev, 244, 0x00);
+
+	rt2800_bbp_write(rt2x00dev, 158, 0x00);
+	rt2800_bbp_write(rt2x00dev, 159, 0x00);
+	rt2800_bbp_write(rt2x00dev, 158, 0xB0);
+	rt2800_bbp_write(rt2x00dev, 159, 0x00);
+
+	rt2800_bbp_write(rt2x00dev, 30, bbpr30);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 39, rfb0r39);
+	rt2800_rfcsr_write_bank(rt2x00dev, 0, 42, rfb0r42);
+
+	if (test_bit(CAPABILITY_EXTERNAL_PA_TX0, &rt2x00dev->cap_flags)) {
+		rt2800_bbp_write(rt2x00dev, 4, bbpr4);
+	}
+
+	rt2800_bbp_write(rt2x00dev, 21, 0x01);
+	udelay(1);
+	rt2800_bbp_write(rt2x00dev, 21, 0x00);
+
+	rt2800_rf_configrecover(rt2x00dev, rf_store);
+
+	rt2800_register_write(rt2x00dev, TX_PIN_CFG, macorg1);
+	rt2800_register_write(rt2x00dev, RF_CONTROL0, 0x00);
+	rt2800_register_write(rt2x00dev, RF_BYPASS0, 0x00);
+	rt2800_register_write(rt2x00dev, RF_CONTROL0, macorg2);
+	udelay(1);
+	rt2800_register_write(rt2x00dev, RF_BYPASS0, macorg3);
+	rt2800_register_write(rt2x00dev, RF_CONTROL3, macorg4);
+	rt2800_register_write(rt2x00dev, RF_BYPASS3, macorg5);
+	rt2800_register_write(rt2x00dev, MAC_SYS_CTRL, savemacsysctrl);
+	rt2800_register_write(rt2x00dev, 0x13b8, mac13b8);
+
+	rt2x00_info(rt2x00dev, "TX IQ Calibration Done!\n");
+
+	return;
+}
+EXPORT_SYMBOL_GPL(rt2800_loft_iq_calibration);
+
 static void rt2800_bbp_core_soft_reset(struct rt2x00_dev *rt2x00dev,
 				       bool set_bw, bool is_ht40)
 {
@@ -9612,6 +10560,7 @@ static void rt2800_init_rfcsr_6352(struc
 	rt2800_rxdcoc_calibration(rt2x00dev);
 	rt2800_bw_filter_calibration(rt2x00dev, true);
 	rt2800_bw_filter_calibration(rt2x00dev, false);
+	rt2800_loft_iq_calibration(rt2x00dev);
 	rt2800_rxiq_calibration(rt2x00dev);
 }
 
--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.h
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.h
@@ -28,6 +28,16 @@
 #define WCID_START	33
 #define WCID_END	222
 #define STA_IDS_SIZE	(WCID_END - WCID_START + 2)
+#define CHAIN_0		0x0
+#define CHAIN_1		0x1
+#define RF_ALC_NUM	6
+#define CHAIN_NUM	2
+
+typedef struct rf_reg_pair {
+	u8 bank;
+	u8 reg;
+	u8 value;
+} rf_reg_pair;
 
 /* RT2800 driver data structure */
 struct rt2800_drv_data {
@@ -248,6 +258,7 @@ int rt2800_calcrcalibrationcode(struct r
 void rt2800_r_calibration(struct rt2x00_dev *rt2x00dev);
 void rt2800_rxdcoc_calibration(struct rt2x00_dev *rt2x00dev);
 void rt2800_rxiq_calibration(struct rt2x00_dev *rt2x00dev);
+void rt2800_loft_iq_calibration(struct rt2x00_dev *rt2x00dev);
 
 int rt2800_enable_radio(struct rt2x00_dev *rt2x00dev);
 void rt2800_disable_radio(struct rt2x00_dev *rt2x00dev);
--- a/drivers/net/wireless/ralink/rt2x00/rt2x00.h
+++ b/drivers/net/wireless/ralink/rt2x00/rt2x00.h
@@ -577,6 +577,7 @@ struct rt2x00lib_ops {
 	void (*r_calibration) (struct rt2x00_dev *rt2x00dev);
 	void (*rxdcoc_calibration) (struct rt2x00_dev *rt2x00dev);
 	void (*rxiq_calibration) (struct rt2x00_dev *rt2x00dev);
+	void (*loft_iq_calibration) (struct rt2x00_dev *rt2x00dev);
 
 	/*
 	 * Data queue handlers.
