From bda176cceb735b9b46c1900658b6486c34e13ae6 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Marek=20Beh=C3=BAn?= <kabel@kernel.org>
Date: Mon, 4 Jul 2022 12:59:54 +0200
Subject: [PATCH] leds: turris-omnia: initialize multi-intensity to full
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The default color of each LED before driver probe (255, 255, 255).
Initialize multi_intensity to this value, so that it corresponds to the
reality.

Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/leds/leds-turris-omnia.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/leds/leds-turris-omnia.c
+++ b/drivers/leds/leds-turris-omnia.c
@@ -131,10 +131,13 @@ static int omnia_led_register(struct i2c
 	}
 
 	led->subled_info[0].color_index = LED_COLOR_ID_RED;
+	led->subled_info[0].intensity = 255;
 	led->subled_info[0].channel = 0;
 	led->subled_info[1].color_index = LED_COLOR_ID_GREEN;
+	led->subled_info[1].intensity = 255;
 	led->subled_info[1].channel = 1;
 	led->subled_info[2].color_index = LED_COLOR_ID_BLUE;
+	led->subled_info[2].intensity = 255;
 	led->subled_info[2].channel = 2;
 
 	led->mc_cdev.subled_info = led->subled_info;
