// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca953x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "tplink,tl-wa850re-v2", "qca,qca9533";
	model = "TP-Link TL-WA850RE v2";

	aliases {
		led-boot = &led_re;
		led-failsafe = &led_re;
		led-running = &led_re;
		led-upgrade = &led_re;
		label-mac-device = &wmac;
	};

	leds {
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		lan {
			label = "blue:lan";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		led_re: re {
			label = "blue:re";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		signal1 {
			label = "blue:signal1";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		signal2 {
			label = "blue:signal2";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		signal3 {
			label = "blue:signal3";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		signal4 {
			label = "blue:signal4";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		led_signal5: signal5 {
			label = "blue:signal5";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "blue:wlan";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "WPS button";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio {
	led_enable {
		gpio-hog;
		gpios = <15 GPIO_ACTIVE_HIGH>;
		line-name = "tp-link:power:led";
		output-high;
	};
};

&spi {
	status = "okay";

	flash@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x020000 0x390000>;
				compatible = "tplink,firmware";
			};

			partition@3b0000 {
				label = "partition-table";
				reg = <0x3b0000 0x010000>;
				read-only;
			};

			info: partition@3c0000 {
				label = "info";
				reg = <0x3c0000 0x010000>;
				read-only;
			};

			partition@3d0000 {
				label = "config";
				reg = <0x3d0000 0x020000>;
				read-only;
			};

			art: partition@3f0000 {
				label = "art";
				reg = <0x3f0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy4>;

	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	compatible = "syscon", "simple-mfd";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";
};

&info {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_info_8: macaddr@8 {
		reg = <0x8 0x6>;
	};
};
