--- /dev/null
+++ b/backport-include/linux/bcma/bcma_driver_chipcommon.h
@@ -0,0 +1,10 @@
+#ifndef __BACKPORT_BCMA_DRIVER_CHIPCOMMON_H
+#define __BACKPORT_BCMA_DRIVER_CHIPCOMMON_H
+
+#include_next <linux/bcma/bcma_driver_chipcommon.h>
+
+#ifndef BCMA_CC_SROM_CONTROL_OTP_PRESENT
+#define BCMA_CC_SROM_CONTROL_OTP_PRESENT 0x00000020
+#endif
+
+#endif
