// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include "armada-385.dtsi"

/ {
	model = "Fortinet FortiGate 50E";
	compatible = "fortinet,fg-50e", "marvell,armada385", "marvell,armada380";

	aliases {
		led-boot = &led_status_green;
		led-failsafe = &led_status_red;
		led-running = &led_status_green;
		led-upgrade = &led_status_green;
		label-mac-device = &eth0;
	};

	chosen {
		stdout-path = "serial0:9600n8";
	};

	memory@0 {
		device_type = "memory";
		reg = <0x00000000 0x80000000>; /* 2GB */
	};

	soc {
		ranges = <MBUS_ID(0xf0, 0x01) 0 0xf1000000 0x100000
			  MBUS_ID(0x01, 0x1d) 0 0xfff00000 0x100000
			  MBUS_ID(0x09, 0x19) 0 0xf1100000 0x10000
			  MBUS_ID(0x09, 0x15) 0 0xf1110000 0x10000
			  MBUS_ID(0x0c, 0x04) 0 0xf1200000 0x100000>;
	};

	gpio-keys {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&pmx_gpio_keys_pins>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio1 22 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&pmx_gpio_leds_pins>;

		led-0 {
			label = "red:alarm";
			gpios = <&gpio0 30 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_ALARM;
		};

		led-1 {
			label = "red:ha";
			gpios = <&gpio1 0 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
		};

		led_status_green: led-2 {
			label = "green:sta";
			gpios = <&gpio1 1 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
		};

		led-3 {
			label = "green:ha";
			gpios = <&gpio1 3 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
		};

		led-4 {
			label = "amber:alarm";
			gpios = <&gpio1 13 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_ALARM;
		};

		led_status_red: led-5 {
			label = "red:sta";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
		};

		led-6 {
			label = "green:speed_wan1";
			gpios = <&gpio2 0 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			linux,default-trigger = "f1072004.mdio-mii:00:1Gbps";
		};

		led-7 {
			label = "green:speed_wan2";
			gpios = <&gpio2 1 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			linux,default-trigger = "f1072004.mdio-mii:01:1Gbps";
		};

		led-8 {
			label = "amber:speed_lan5";
			gpios = <&gpio2 2 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_AMBER>;
			linux,default-trigger = "mv88e6xxx-1:00:100Mbps";
		};

		led-9 {
			label = "green:speed_lan5";
			gpios = <&gpio2 3 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_GREEN>;
			linux,default-trigger = "mv88e6xxx-1:00:1Gbps";
		};

		led-10 {
			label = "green:speed_lan4";
			gpios = <&gpio2 4 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			linux,default-trigger = "mv88e6xxx-1:01:1Gbps";
		};

		led-11 {
			label = "amber:speed_lan4";
			gpios = <&gpio2 5 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			linux,default-trigger = "mv88e6xxx-1:01:100Mbps";
		};

		led-12 {
			label = "amber:speed_lan3";
			gpios = <&gpio2 6 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			linux,default-trigger = "mv88e6xxx-1:02:100Mbps";
		};

		led-13 {
			label = "green:speed_lan3";
			gpios = <&gpio2 7 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			linux,default-trigger = "mv88e6xxx-1:02:1Gbps";
		};

		led-14 {
			label = "green:speed_lan1";
			gpios = <&gpio2 12 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			linux,default-trigger = "mv88e6xxx-1:04:1Gbps";
		};

		led-15 {
			label = "amber:speed_lan1";
			gpios = <&gpio2 13 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			linux,default-trigger = "mv88e6xxx-1:04:100Mbps";
		};

		led-16 {
			label = "green:speed_lan2";
			gpios = <&gpio2 14 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			linux,default-trigger = "mv88e6xxx-1:03:1Gbps";
		};

		led-17 {
			label = "amber:speed_lan2";
			gpios = <&gpio2 15 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			linux,default-trigger = "mv88e6xxx-1:03:100Mbps";
		};
	};

	reg_usb_vbus: regulator-usb-vbus {
		compatible = "fixed-regulator";
		regulator-name = "usb-vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio1 21 GPIO_ACTIVE_LOW>;
		regulator-always-on;
	};
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0_pins>;
	status = "okay";

	gpio2: gpio@24 {
		compatible = "nxp,pca9555";
		reg = <0x24>;
		gpio-controller;
		#gpio-cells = <0x2>;
	};

	hwmon@28 {
		compatible = "nuvoton,nct7802";
		reg = <0x28>;
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins>;
	status = "okay";
};

&pinctrl {
	pmx_phy_switch_pins: phy-switch-pins {
		marvell,pins = "mpp19", "mpp20", "mpp23", "mpp34", "mpp41";
		marvell,function = "gpio";
	};

	pmx_gpio_leds_pins: gpio-leds-pins {
		marvell,pins = "mpp30", "mpp32", "mpp33", "mpp35",
			       "mpp45", "mpp47";
		marvell,function = "gpio";
	};

	pmx_usb_pins: usb-pins {
		marvell,pins = "mpp53";
		marvell,function = "gpio";
	};

	pmx_gpio_keys_pins: gpio-keys-pins {
		marvell,pins = "mpp54";
		marvell,function = "gpio";
	};
};

&bm {
	status = "okay";
};

&bm_bppi {
	status = "okay";
};

&eth0 {
	pinctrl-names = "default";
	pinctrl-0 = <&ge0_rgmii_pins>;
	status = "okay";

	phy-connection-type = "rgmii-id";
	buffer-manager = <&bm>;
	bm,pool-long = <0>;
	bm,pool-short = <1>;
	nvmem-cells = <&macaddr_bdinfo_d880>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&eth1 {
	status = "okay";

	phy-handle = <&ethphy0>;
	phy-connection-type = "sgmii";
	buffer-manager = <&bm>;
	bm,pool-long = <2>;
	nvmem-cells = <&macaddr_bdinfo_d880>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <1>;
};

&eth2 {
	status = "okay";

	phy-handle = <&ethphy1>;
	phy-connection-type = "sgmii";
	buffer-manager = <&bm>;
	bm,pool-long = <3>;
	nvmem-cells = <&macaddr_bdinfo_d880>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <2>;
};

&mdio {
	pinctrl-names = "default";
	pinctrl-0 = <&mdio_pins>, <&pmx_phy_switch_pins>;

	/* Marvell 88E1512 */
	ethphy0: ethernet-phy@0 {
		compatible = "ethernet-phy-id0141,0dd1",
			     "ethernet-phy-ieee802.3-c22";
		reg = <0>;
		interrupt-parent = <&gpio0>;
		interrupts = <20 IRQ_TYPE_LEVEL_LOW>;
		reset-gpios = <&gpio0 23 GPIO_ACTIVE_LOW>;
		reset-assert-us = <10000>;
		reset-deassert-us = <10000>;
		/*
		 * LINK/ACT   (Green): LED[0], Active Low
		 * SPEED 100M (Amber): LED[1], Active High
		 */
		marvell,reg-init = <3 16 0 0x71>,
				   <3 17 0 0x4>;
	};

	/* Marvell 88E1512 */
	ethphy1: ethernet-phy@1 {
		compatible = "ethernet-phy-id0141,0dd1",
			     "ethernet-phy-ieee802.3-c22";
		reg = <1>;
		interrupt-parent = <&gpio1>;
		interrupts = <9 IRQ_TYPE_LEVEL_LOW>;
		reset-gpios = <&gpio1 2 GPIO_ACTIVE_LOW>;
		reset-assert-us = <10000>;
		reset-deassert-us = <10000>;
		/*
		 * LINK/ACT   (Green): LED[0], Active Low
		 * SPEED 100M (Amber): LED[1], Active High
		 */
		marvell,reg-init = <3 16 0 0x71>,
				   <3 17 0 0x4>;
	};

	/* Marvell 88E6176 */
	switch@2 {
		compatible = "marvell,mv88e6085";
		reg = <0x2>;
		reset-gpios = <&gpio0 19 GPIO_ACTIVE_LOW>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "lan5";
				nvmem-cells = <&macaddr_bdinfo_d880>;
				nvmem-cell-names = "mac-address";
				mac-address-increment = <7>;
			};

			port@1 {
				reg = <1>;
				label = "lan4";
				nvmem-cells = <&macaddr_bdinfo_d880>;
				nvmem-cell-names = "mac-address";
				mac-address-increment = <6>;
			};

			port@2 {
				reg = <2>;
				label = "lan3";
				nvmem-cells = <&macaddr_bdinfo_d880>;
				nvmem-cell-names = "mac-address";
				mac-address-increment = <5>;
			};

			port@3 {
				reg = <3>;
				label = "lan2";
				nvmem-cells = <&macaddr_bdinfo_d880>;
				nvmem-cell-names = "mac-address";
				mac-address-increment = <4>;
			};

			port@4 {
				reg = <4>;
				label = "lan1";
				nvmem-cells = <&macaddr_bdinfo_d880>;
				nvmem-cell-names = "mac-address";
				mac-address-increment = <3>;
			};

			port@6 {
				reg = <6>;
				ethernet = <&eth0>;
				phy-connection-type = "rgmii-id";

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};
	};
};

&usb3_0 {
	pinctrl-names = "default";
	pinctrl-0 = <&pmx_usb_pins>;
	status = "okay";

	vbus-supply = <&reg_usb_vbus>;
};

&spi1 {
	pinctrl-names = "default";
	pinctrl-0 = <&spi1_pins>;
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x1c0000>;
				label = "u-boot";
				read-only;
			};

			partition@1c0000 {
				reg = <0x1c0000 0x10000>;
				label = "firmware-info";

				/*
				 *  0x10 - 0x2f : image name (image1)
				 *  0x30 - 0x4f : image name (image2)
				 * 0x170 (1byte): active image (0x0/0x1)
				 * 0x184 - 0x185: kernel block count (image1)
				 * 0x18c - 0x18d: rootfs block count (image1)
				 * 0x194 - 0x195: kernel block count (image2)
				 * 0x19c - 0x19d: rootfs block count (image2)
				 * 0x1be (1byte): bit7 -> active flag (image1)?
				 * 0x1ce (1byte): bit7 -> active flag (image2)?
				 *
				 * Note: block size --> 0x200 (512 bytes)
				 */
			};

			partition@1d0000 {
				reg = <0x1d0000 0x10000>;
				label = "dtb";
				read-only;
			};

			partition@1e0000 {
				reg = <0x1e0000 0x10000>;
				label = "u-boot-env";
				read-only;
			};

			partition@1f0000 {
				reg = <0x1f0000 0x10000>;
				label = "board-info";
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_bdinfo_d880: macaddr@d880 {
					reg = <0xd880 0x6>;
				};
			};

			partition@200000 {
				reg = <0x200000 0x600000>;
				label = "kernel";
			};

			partition@800000 {
				reg = <0x800000 0x1800000>;
				label = "rootfs";
			};

			partition@2000000 {
				reg = <0x2000000 0x600000>;
				label = "kn2";
				read-only;
			};

			partition@2600000 {
				reg = <0x2600000 0x1800000>;
				label = "rfs2";
				read-only;
			};

			partition@3e00000 {
				reg = <0x3e00000 0x1200000>;
				label = "part1";
				read-only;
			};

			partition@5000000 {
				reg = <0x5000000 0x1200000>;
				label = "part2";
				read-only;
			};

			partition@6200000 {
				reg = <0x6200000 0x1e00000>;
				label = "config";
				read-only;
			};
		};
	};
};
