From 18be654a4345f7d937b4bfbad74bea8093e3a93c Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Wed, 2 Feb 2022 01:03:26 +0100
Subject: [PATCH 07/16] net: dsa: tag_qca: add define for handling MIB packet

Add struct to correctly parse a mib Ethernet packet.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 include/linux/dsa/tag_qca.h | 10 ++++++++++
 net/dsa/tag_qca.c           |  4 ++++
 2 files changed, 14 insertions(+)

--- a/include/linux/dsa/tag_qca.h
+++ b/include/linux/dsa/tag_qca.h
@@ -62,4 +62,14 @@ struct qca_mgmt_ethhdr {
 	__be16 hdr;		/* qca hdr */
 } __packed;
 
+enum mdio_cmd {
+	MDIO_WRITE = 0x0,
+	MDIO_READ
+};
+
+struct mib_ethhdr {
+	u32 data[3];		/* first 3 mib counter */
+	__be16 hdr;		/* qca hdr */
+} __packed;
+
 #endif /* __TAG_QCA_H */
--- a/net/dsa/tag_qca.c
+++ b/net/dsa/tag_qca.c
@@ -57,6 +57,10 @@ static struct sk_buff *qca_tag_rcv(struc
 	if (pk_type == QCA_HDR_RECV_TYPE_RW_REG_ACK)
 		return NULL;
 
+	/* Ethernet MIB counter packet */
+	if (pk_type == QCA_HDR_RECV_TYPE_MIB)
+		return NULL;
+
 	/* Remove QCA tag and recalculate checksum */
 	skb_pull_rcsum(skb, QCA_HDR_LEN);
 	dsa_strip_etype_header(skb, QCA_HDR_LEN);
