
. /lib/functions/system.sh
. /lib/functions/uci-defaults.sh
. /lib/functions/k2t.sh

ath79_setup_interfaces()
{
	local board="$1"

	case "$board" in
	adtran,bsap1800-v2|\
	adtran,bsap1840|\
	allnet,all-wap02860ac|\
	alfa-network,ap121f|\
	alfa-network,pi-wifi4|\
	alfa-network,tube-2hq|\
	araknis,an-300-ap-i-n|\
	araknis,an-500-ap-i-ac|\
	araknis,an-700-ap-i-ac|\
	arduino,yun|\
	aruba,ap-105|\
	aruba,ap-175|\
	asus,rp-ac51|\
	asus,rp-ac66|\
	avm,fritz1750e|\
	avm,fritz300e|\
	avm,fritzdvbc|\
	comfast,cf-wr752ac-v1|\
	comfast,cf-e130n-v2|\
	devolo,dvl1200i|\
	devolo,dvl1750c|\
	devolo,dvl1750i|\
	devolo,dvl1750x|\
	dlink,dap-1330-a1|\
	dlink,dap-1365-a1|\
	dlink,dap-2230-a1|\
	dlink,dap-2660-a1|\
	dlink,dap-2680-a1|\
	dlink,dap-3320-a1|\
	dlink,dir-505|\
	engenius,eap1200h|\
	engenius,eap1750h|\
	engenius,eap600|\
	engenius,ecb1200|\
	engenius,ecb1750|\
	engenius,ecb600|\
	enterasys,ws-ap3705i|\
	extreme-networks,ws-ap3805i|\
	fortinet,fap-221-b|\
	glinet,gl-ar300m-lite|\
	glinet,gl-usb150|\
	hak5,wifi-pineapple-nano|\
	meraki,mr16|\
	netgear,ex7300|\
	netgear,ex7300-v2|\
	netgear,wndap360|\
	ocedo,koala|\
	ocedo,raccoon|\
	onion,omega|\
	openmesh,mr600-v1|\
	openmesh,mr600-v2|\
	openmesh,mr900-v1|\
	openmesh,mr900-v2|\
	openmesh,mr1750-v1|\
	openmesh,mr1750-v2|\
	pcs,cap324|\
	pisen,ts-d084|\
	pisen,wmb001n|\
	pisen,wmm003n|\
	ruckus,zf7321|\
	ruckus,zf7341|\
	ruckus,zf7351|\
	siemens,ws-ap3610|\
	sophos,ap15|\
	sophos,ap55|\
	sophos,ap55c|\
	sophos,ap100|\
	sophos,ap100c|\
	tplink,cpe210-v2|\
	tplink,cpe210-v3|\
	tplink,cpe510-v2|\
	tplink,cpe510-v3|\
	tplink,cpe605-v1|\
	tplink,cpe610-v1|\
	tplink,cpe610-v2|\
	tplink,cpe710-v1|\
	tplink,eap225-outdoor-v1|\
	tplink,eap225-outdoor-v3|\
	tplink,eap225-v1|\
	tplink,eap225-v3|\
	tplink,eap225-v4|\
	tplink,eap245-v1|\
	tplink,re350k-v1|\
	tplink,re355-v1|\
	tplink,re450-v1|\
	tplink,re450-v2|\
	tplink,re450-v3|\
	tplink,re455-v1|\
	tplink,tl-wa1201-v2|\
	tplink,tl-wr902ac-v1|\
	ubnt,bullet-ac|\
	ubnt,bullet-m-xw|\
	ubnt,lap-120|\
	ubnt,litebeam-ac-gen2|\
	ubnt,nanobeam-ac|\
	ubnt,nanobeam-ac-xc|\
	ubnt,nanostation-ac-loco|\
	ubnt,nanostation-loco-m-xw|\
	ubnt,powerbeam-5ac-500|\
	ubnt,powerbeam-5ac-gen2|\
	ubnt,powerbeam-m2-xw|\
	ubnt,powerbeam-m5-xw|\
	ubnt,powerbridge-m|\
	ubnt,rocket-5ac-lite|\
	ubnt,rocket-m|\
	ubnt,unifiac-lite|\
	ubnt,unifiac-lr|\
	ubnt,unifiac-mesh|\
	ubnt,unifi|\
	watchguard,ap100|\
	watchguard,ap200|\
	watchguard,ap300|\
	wd,mynet-wifi-rangeextender|\
	winchannel,wb2000|\
	zyxel,nwa1100-nh|\
	zyxel,nwa1121-ni|\
	zyxel,nwa1123-ac|\
	zyxel,nwa1123-ni)
		ucidef_set_interface_lan "eth0"
		;;
	airtight,c-75)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:wan" "3:lan" "6@eth1"
		;;
	alfa-network,ap121fe)
		ucidef_set_interface_lan "eth0 usb0"
		;;
	alfa-network,n2q|\
	alfa-network,n5q|\
	devolo,dvl1200e|\
	devolo,dvl1750e|\
	engenius,enstationac-v1|\
	engenius,ews511ap|\
	engenius,ews660ap|\
	ocedo,ursus|\
	ruckus,zf7363|\
	ruckus,zf7372|\
	ubnt,unifi-ap-outdoor-plus)
		ucidef_set_interface_lan "eth0 eth1"
		;;
	asus,pl-ac56)
		# port 6 (internal) is the power-line port
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "2:lan:2" "3:lan:3" "6:lan:4"
		;;
	atheros,db120)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan" "4:lan" "5:lan" "1:wan"
		ucidef_add_switch "switch1" \
			"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan" "5:lan"
		;;
	avm,fritz4020|\
	pcs,cr3000|\
	tplink,archer-c58-v1|\
	tplink,archer-c59-v1|\
	tplink,archer-c59-v2|\
	wd,mynet-n600)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "2:lan:4" "3:lan:3" "4:lan:2"
		;;
	belkin,f9j1108-v2|\
	belkin,f9k1115-v2|\
	tplink,archer-c5-v1|\
	tplink,archer-c7-v1|\
	tplink,archer-c7-v2|\
	tplink,tl-wdr4900-v2|\
	tplink,tl-wdr7500-v3)
		ucidef_add_switch "switch0" \
			"0@eth1" "2:lan" "3:lan" "4:lan" "5:lan" "6@eth0" "1:wan"
		;;
	buffalo,bhr-4grv|\
	buffalo,wzr-hp-g450h)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan" "4:lan" "5:lan" "1:wan"
		;;
	buffalo,bhr-4grv2|\
	trendnet,tew-823dru)
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan" "6@eth0"
		;;
	buffalo,wzr-600dhp|\
	buffalo,wzr-hp-ag300h|\
	tplink,archer-c25-v1|\
	tplink,archer-c60-v1|\
	tplink,archer-c60-v2|\
	tplink,archer-c60-v3|\
	tplink,tl-wdr3500-v1|\
	tplink,tl-wr842n-v1|\
	tplink,tl-wr842n-v3)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	teltonika,rut300)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "2:lan:4" "3:lan:3" "4:lan:2"
		;;
	buffalo,wzr-hp-g300nh-rb|\
	buffalo,wzr-hp-g300nh-s|\
	dlink,dir-825-b1|\
	trendnet,tew-673gru)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0:lan" "1:lan" "2:lan" "3:lan" "5@eth0"
		;;
	buffalo,wzr-hp-g302h-a1a0)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "3:lan:4" "4:lan:3" "5:lan:2" "2:wan"
		;;
	alcatel,hh40v|\
	comfast,cf-e110n-v2|\
	comfast,cf-e120a-v3|\
	comfast,cf-e314n-v2|\
	compex,wpj531-16m|\
	openmesh,a40|\
	openmesh,a60|\
	openmesh,om2p-v1|\
	openmesh,om2p-v4|\
	openmesh,om2p-hs-v4|\
	plasmacloud,pa300|\
	plasmacloud,pa300e|\
	tplink,cpe210-v1|\
	tplink,cpe220-v2|\
	tplink,cpe220-v3|\
	tplink,cpe510-v1|\
	tplink,wbs210-v1|\
	tplink,wbs210-v2|\
	tplink,wbs510-v1|\
	tplink,wbs510-v2|\
	ubnt,routerstation)
		ucidef_set_interfaces_lan_wan "eth1" "eth0"
		;;
	comfast,cf-e375ac)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:wan" "2:lan"
		;;
	comfast,cf-e560ac|\
	qca,ap143-8m|\
	qca,ap143-16m|\
	tplink,tl-wr841hp-v3)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan"
		;;
	comfast,cf-wr650ac-v1|\
	comfast,cf-wr650ac-v2|\
	zyxel,nbg6616)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan" "6@eth1"
		;;
	compex,wpj344-16m|\
	compex,wpj563)
		ucidef_add_switch "switch0" \
			"0@eth0" "3:lan" "2:wan"
		;;
	compex,wpj558-16m)
		ucidef_add_switch "switch0" \
			"1:wan" "5:lan" "6@eth0"
		;;
	devolo,dlan-pro-1200plus-ac|\
	devolo,magic-2-wifi)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:wan" "3:lan" "4:lan"
		;;
	dlink,dap-2695-a1)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:wan" "6@eth1"
		;;
	dlink,dap-3662-a1)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:2" "2:lan:1" "6@eth1"
		;;
	dlink,dch-g020-a1)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:2" "2:lan:1"
		;;
	dlink,dir-629-a1|\
	dlink,dir-825-c1|\
	dlink,dir-835-a1|\
	dlink,dir-842-c1|\
	dlink,dir-842-c2|\
	dlink,dir-842-c3|\
	dlink,dir-859-a1|\
	dlink,dir-859-a3|\
	dlink,dir-869-a1|\
	engenius,epg5000|\
	engenius,esr1200|\
	engenius,esr1750|\
	engenius,esr900|\
	sitecom,wlr-7100|\
	tplink,archer-c2-v3|\
	tplink,tl-wr1043nd-v4|\
	tplink,tl-wr1043n-v5)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5:wan"
		;;
	elecom,wrc-1750ghbk2-i|\
	elecom,wrc-300ghbk2-i|\
	sitecom,wlr-8100)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:4" "3:lan:3" "4:lan:2" "5:lan:1" "1:wan"
		;;
	embeddedwireless,balin)
		ucidef_add_switch "switch0" \
			"0@eth0" "5:lan:1" "4:lan:2" "3:wan"
		;;
	embeddedwireless,dorin)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:wan" "2:lan:3" "3:lan:2"
		;;
	engenius,eap300-v2)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan"
		;;
	engenius,ens202ext-v1)
		ucidef_set_interface_lan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan"
		;;
	etactica,eg200)
		ucidef_set_interface_lan "eth0" "dhcp"
		;;
	glinet,gl-ar750)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan"
		;;
	glinet,gl-x300b)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "4:lan"
		;;
	iodata,etg3-r|\
	iodata,wn-ac1167dgr|\
	iodata,wn-ac1600dgr|\
	iodata,wn-ac1600dgr2|\
	iodata,wn-ag300dgr|\
	pcs,cr5000|\
	wd,mynet-n750)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan"
		;;
	jjplus,jwap230)
		ucidef_add_switch "switch0" \
			"0@eth0" "5:wan:1" "1:lan:2" "6@eth1"
		;;
	joyit,jt-or750i)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	kuwfi,c910)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:2" "4:lan:1"
		;;
	letv,lba-047-ch)
		ucidef_set_interface_wan "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "3:lan:2" "4:lan:1"
		;;
	librerouter,librerouter-v1)
		ucidef_add_switch "switch0" \
			"0@eth0" "5:wan" "6@eth1" "4:lan"
		;;
	meraki,mr12)
		ucidef_set_interface_lan "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan"
		;;
	mercury,mw4530r-v1|\
	tplink,archer-a7-v5|\
	tplink,archer-a9-v6|\
	tplink,archer-c6-v2|\
	tplink,archer-c6-v2-us|\
	tplink,archer-c7-v4|\
	tplink,archer-c7-v5|\
	tplink,tl-wdr3600-v1|\
	tplink,tl-wdr4300-v1|\
	tplink,tl-wdr4300-v1-il|\
	tplink,tl-wdr4310-v1)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "3:lan:2" "4:lan:3" "5:lan:4" "1:wan"
		;;
	nec,wf1200cr)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan"
		;;
	nec,wg1200cr|\
	qxwlan,e1700ac-v2-8m|\
	qxwlan,e1700ac-v2-16m|\
	qxwlan,e750g-v8-8m|\
	qxwlan,e750g-v8-16m|\
	ubnt,nanobeam-ac-gen2|\
	ubnt,nanostation-ac|\
	yuncore,a782|\
	yuncore,xd3200|\
	yuncore,xd4200)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:wan"
		;;
	nec,wg800hp|\
	xiaomi,aiot-ac2350)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan" "4:lan" "1:wan"
		;;
	netgear,wndr3700|\
	netgear,wndr3700-v2|\
	netgear,wndr3800|\
	netgear,wndr3800ch|\
	netgear,wndrmac-v1|\
	netgear,wndrmac-v2)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5u@eth0"
		ucidef_add_switch_attr "switch0" "blinkrate" 2
		ucidef_add_switch_port_attr "switch0" 1 led 6
		ucidef_add_switch_port_attr "switch0" 2 led 9
		ucidef_add_switch_port_attr "switch0" 5 led 2
		;;
	netgear,wnr2200-8m|\
	netgear,wnr2200-16m)
		ucidef_set_interface_wan "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan" "2:lan" "3:lan" "4:lan"
		;;
	phicomm,k2t)
		ucidef_add_switch "switch0" \
			"0@eth0" "3:lan:1" "5:lan:2" "4:wan"
		;;
	qihoo,c301)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan" "3:lan"
		;;
	qxwlan,e558-v2-8m|\
	qxwlan,e558-v2-16m)
		ucidef_add_switch "switch0" \
			"0@eth1" "4:lan" "5:lan" "6@eth0" "3:wan"
		;;
	rosinson,wr818)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:wan"
		;;
	ruckus,zf7025)
		ucidef_set_interface_lan "eth0 eth1"
		ucidef_add_switch "switch0" \
			"0u@eth1" "4:lan:1" "3:lan:2" "2:lan:3" "1:lan:4"
		;;
	teltonika,rut955|\
	teltonika,rut955-h7v3c0)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	tplink,archer-d50-v1)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:3" "3:lan:2" "4:lan:1" "1:wan"
		;;
	tplink,archer-d7-v1|\
	tplink,archer-d7b-v1)
		ucidef_add_switch "switch0" \
			"0@eth1" "3:lan:3" "4:lan:2" "5:lan:1" "6@eth0" "2:wan:4" "1:wan:5"
		;;
	tplink,eap225-wall-v2)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan"
		;;
	tplink,eap245-v3)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "5:lan:2"
		;;
	tplink,tl-mr6400-v1)
		ucidef_set_interfaces_lan_wan "eth0.1 eth1" "usb0"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:1" "2:lan:3" "3:lan:2"
		;;
	tplink,tl-wpa8630-v1)
		# port 5 (internal) is the power-line port
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:3" "3:lan:2" "4:lan:1" "5:lan:4"
		;;
	tplink,tl-wr841hp-v2|\
	tplink,tl-wr842n-v2|\
	tplink,tl-wr941hp-v1)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan:4" "2:lan:1" "3:lan:2" "4:lan:3"
		;;
	tplink,tl-wr1043nd-v1)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "5@eth0"
		;;
	tplink,tl-wr1043nd-v2|\
	tplink,tl-wr1043nd-v3|\
	tplink,tl-wr1045nd-v2)
		ucidef_add_switch "switch0" \
			"0@eth1" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5:wan" "6@eth0"
		;;
	tplink,tl-wr2543-v1)
		ucidef_add_switch "switch0" \
			"1:lan" "2:lan" "3:lan" "4:lan" "0:wan" "9@eth0"
		;;
	ubnt,aircube-ac)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "3:lan:2" "5:lan:3" "4:wan"
		;;
	ubnt,aircube-isp)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "3:lan:3" "4:lan:2"
		;;
	ubnt,edgeswitch-5xp)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan" "5:lan"
		;;
	ubnt,edgeswitch-8xp)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0:lan:1" "1:lan:2" "2:lan:3" "3:lan:4" "4:lan:5" "5:lan:6" "6:lan:7" "7:lan:8"  "8@eth0"
		;;
	ubnt,routerstation-pro)
		ucidef_set_interface_wan "eth0"
		ucidef_add_switch "switch0" \
			"0@eth1" "2:lan:3" "3:lan:2" "4:lan:1"
		;;
	ubnt,nanostation-m-xw)
		ucidef_add_switch "switch0" \
			"0@eth0" "5:lan" "1:wan"
		;;
	ubnt,unifiac-mesh-pro|\
	ubnt,unifiac-pro)
		ucidef_add_switch "switch0" \
			"0@eth0" "2:lan:1" "3:lan:2"
		;;
	ubnt,unifi-ap-pro)
		ucidef_add_switch "switch0" \
			"0@eth0" "1:lan" "2:lan"
		;;
	tplink,deco-m4r-v1|\
	tplink,deco-s4-v2)
		ucidef_add_switch "switch0" \
			"0@eth0" "3:lan:1" "5:lan:2"
		;;
	hiwifi,hc6361|\
	xiaomi,mi-router-4q|\
	zbtlink,zbt-wd323)
		ucidef_set_interface_wan "eth1"
		ucidef_add_switch "switch0" \
			"0@eth0" "3:lan:1" "4:lan:2"
		;;
	*)
		ucidef_set_interfaces_lan_wan "eth0" "eth1"
		;;
	esac
}

ath79_setup_macs()
{
	local board="$1"

	case "$board" in
	adtran,bsap1800-v2|\
	adtran,bsap1840)
		lan_mac=$(mtd_get_mac_binary "Board data" 2)
		label_mac=$lan_mac
		;;
	alfa-network,ap121f|\
	alfa-network,ap121fe|\
	alfa-network,n2q|\
	alfa-network,n5q|\
	alfa-network,pi-wifi4|\
	alfa-network,r36a|\
	alfa-network,tube-2hq|\
	engenius,eap300-v2|\
	engenius,ens202ext-v1)
		label_mac=$(mtd_get_mac_binary art 0x1002)
		;;
	arduino,yun)
		base_mac=$(mtd_get_mac_binary art 0x1002)
		lan_mac=$(macaddr_setbit $base_mac 29)
		[ $lan_mac = $base_mac ] && lan_mac=$(macaddr_unsetbit $base_mac 29)
		;;
	avm,fritz1750e|\
	avm,fritz450e|\
	avm,fritzdvbc)
		label_mac=$(fritz_tffs -n macwlan -i $(find_mtd_part "tffs (1)"))
		;;
	avm,fritz300e)
		lan_mac=$(fritz_tffs -n maca -i $(find_mtd_part "tffs (1)"))
		label_mac=$(fritz_tffs -n macwlan -i $(find_mtd_part "tffs (1)"))
		;;
	avm,fritz4020)
		lan_mac=$(fritz_tffs -n maca -i $(find_mtd_part "tffs (1)"))
		wan_mac=$(fritz_tffs -n macb -i $(find_mtd_part "tffs (1)"))
		;;
	comfast,cf-e375ac)
		wan_mac=$(macaddr_add $(mtd_get_mac_binary art 0x0) 1)
		;;
	compex,wpj344-16m|\
	compex,wpj558-16m|\
	compex,wpj563)
		wan_mac=$(mtd_get_mac_binary u-boot 0x2e018)
		;;
	devolo,dlan-pro-1200plus-ac|\
	devolo,magic-2-wifi)
		label_mac=$(macaddr_add "$(mtd_get_mac_binary art 0x1002)" 3)
		;;
	dlink,dap-1330-a1|\
	dlink,dap-1365-a1|\
	dlink,dch-g020-a1)
		lan_mac=$(mtd_get_mac_text "mp" 0x1)
		label_mac=$lan_mac
		;;
	dlink,dap-2230-a1|\
	dlink,dap-2660-a1|\
	dlink,dap-2680-a1|\
	dlink,dap-3320-a1)
		lan_mac=$(mtd_get_mac_ascii bdcfg "lanmac")
		label_mac=$lan_mac
		;;
	dlink,dap-2695-a1|\
	dlink,dap-3662-a1)
		label_mac=$(mtd_get_mac_ascii bdcfg "wlanmac")
		;;
	dlink,dir-629-a1)
		wan_mac=$(mtd_get_mac_text "mfcdata" 0x6a)
		;;
	trendnet,tew-673gru)
		lan_mac=$(mtd_get_mac_text "caldata" 0xffa0)
		wan_mac=$(mtd_get_mac_text "caldata" 0xffb4)
		label_mac=$wan_mac
		;;
	dlink,dir-505)
		lan_mac=$(mtd_get_mac_text "mac" 0x4)
		;;
	dlink,dir-825-c1|\
	dlink,dir-835-a1)
		wan_mac=$(mtd_get_mac_text "mac" 0x18)
		;;
	dlink,dir-842-c1|\
	dlink,dir-842-c2|\
	dlink,dir-842-c3)
		lan_mac=$(mtd_get_mac_ascii devdata "lanmac")
		wan_mac=$(mtd_get_mac_ascii devdata "wanmac")
		label_mac=$lan_mac
		;;
	dlink,dir-859-a1|\
	dlink,dir-869-a1)
		lan_mac=$(mtd_get_mac_text "devdata" 0xc9)
		wan_mac=$(mtd_get_mac_text "devdata" 0x79)
		;;
	dlink,dir-859-a3)
		lan_mac=$(get_mac_label)
		wan_mac=$(macaddr_add "$lan_mac" 3)
		;;
	qihoo,c301|\
	wd,mynet-n600|\
	wd,mynet-n750)
		lan_mac=$(mtd_get_mac_ascii devdata "lanmac")
		wan_mac=$(mtd_get_mac_ascii devdata "wanmac")
		;;
	elecom,wrc-1750ghbk2-i|\
	elecom,wrc-300ghbk2-i)
		wan_mac=$(mtd_get_mac_ascii hwconfig "HW.WAN.MAC.Address")
		label_mac=$wan_mac
		;;
	engenius,ecb1200|\
	engenius,ecb1750)
		lan_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		label_mac=$lan_mac
		;;
	engenius,epg5000|\
	engenius,esr1200|\
	engenius,esr1750|\
	engenius,esr900)
		lan_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		wan_mac=$(mtd_get_mac_ascii u-boot-env wanaddr)
		;;
	engenius,ews511ap)
		lan_mac=$(mtd_get_mac_text "u-boot-env" 0xe9)
		eth1_mac=$(macaddr_add "$lan_mac" 1)
		ucidef_set_interface "eth0" ifname "eth0" protocol "none" macaddr "$lan_mac"
		ucidef_set_interface "eth1" ifname "eth1" protocol "none" macaddr "$eth1_mac"
		;;
	enterasys,ws-ap3705i)
		label_mac=$(mtd_get_mac_ascii u-boot-env0 ethaddr)
		;;
	fortinet,fap-221-b)
		lan_mac=$(mtd_get_mac_text u-boot 0x3ff80 12)
		label_mac=$lan_mac
		;;
	hak5,lan-turtle|\
	hak5,packet-squirrel)
		label_mac=$(mtd_get_mac_binary u-boot 0x1fc00)
		;;
	iodata,etg3-r)
		lan_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		wan_mac=$(macaddr_add "$lan_mac" -1)
		label_mac=$wan_mac
		;;
	iodata,wn-ac1167dgr|\
	iodata,wn-ac1600dgr|\
	iodata,wn-ac1600dgr2|\
	iodata,wn-ag300dgr)
		lan_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		wan_mac=$(mtd_get_mac_ascii u-boot-env wanaddr)
		label_mac=$wan_mac
		;;
	mercury,mw4530r-v1|\
	tplink,tl-wdr3600-v1|\
	tplink,tl-wdr4300-v1|\
	tplink,tl-wdr4300-v1-il)
		base_mac=$(mtd_get_mac_binary u-boot 0x1fc00)
		wan_mac=$(macaddr_add "$base_mac" 1)
		;;
	tplink,deco-s4-v2)
		lan_mac=$(mtd_get_mac_encrypted_deco $(find_mtd_part config))
		label_mac=$lan_mac
		;;
	nec,wf1200cr|\
	nec,wg1200cr)
		lan_mac=$(mtd_get_mac_ascii devdata "lanmac")
		wan_mac=$(mtd_get_mac_ascii devdata "wanmac")
		label_mac=$wan_mac
		;;
	nec,wg800hp)
		lan_mac=$(mtd_get_mac_text board_data 0x280)
		wan_mac=$(mtd_get_mac_text board_data 0x480)
		label_mac=$wan_mac
		;;
	netgear,wndr3700|\
	netgear,wndr3700-v2|\
	netgear,wndr3800|\
	netgear,wndrmac-v1|\
	netgear,wndrmac-v2)
		lan_mac=$(macaddr_setbit_la "$(mtd_get_mac_binary art 0x0)")
		;;
	phicomm,k2t)
		lan_mac=$(k2t_get_mac "lan_mac")
		wan_mac=$(k2t_get_mac "wan_mac")
		;;
	rosinson,wr818)
		wan_mac=$(mtd_get_mac_binary factory 0x0)
		lan_mac=$(macaddr_setbit_la "$wan_mac")
		;;
	ruckus,zf7025|\
	ruckus,zf7321|\
	ruckus,zf7341|\
	ruckus,zf7351|\
	ruckus,zf7363|\
	ruckus,zf7372)
		lan_mac=$(mtd_get_mac_binary board-data 0x807E)
		label_mac=$lan_mac
		;;
	sitecom,wlr-7100|\
	sitecom,wlr-8100)
		lan_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		wan_mac=$(mtd_get_mac_ascii u-boot-env wanaddr)
		label_mac=$lan_mac
		;;
	tplink,archer-a7-v5|\
	tplink,archer-a9-v6|\
	tplink,archer-c7-v4|\
	tplink,archer-c7-v5|\
	tplink,tl-wr1043nd-v4|\
	tplink,tl-wr1043n-v5)
		base_mac=$(mtd_get_mac_binary info 0x8)
		wan_mac=$(macaddr_add "$base_mac" 1)
		;;
	trendnet,tew-823dru)
		lan_mac=$(mtd_get_mac_text mac 0x4)
		wan_mac=$(mtd_get_mac_text mac 0x18)
		label_mac=$wan_mac
		;;
	ubnt,powerbridge-m|\
	ubnt,rocket-m|\
	ubnt,unifi)
		label_mac=$(cat /sys/class/ieee80211/phy0/macaddress)
		;;
	ubnt,litebeam-ac-gen2|\
	ubnt,nanobeam-ac-gen2|\
	ubnt,nanobeam-ac-xc|\
	ubnt,powerbeam-5ac-500|\
	ubnt,powerbeam-5ac-gen2)
		label_mac=$(mtd_get_mac_binary art 0x5006)
		;;
	ubnt,routerstation|\
	ubnt,routerstation-pro)
		wan_mac=$(fconfig -s -r -d $(find_mtd_part "RedBoot config") -n ar7100_esa)
		lan_mac=$(macaddr_add "$wan_mac" 1)
		;;
	wd,mynet-wifi-rangeextender)
		lan_mac=$(nvram get et0macaddr)
		;;
	xiaomi,aiot-ac2350)
		lan_mac=$(mtd_get_mac_binary art 0x1002)
		;;
	zyxel,nbg6616)
		label_mac=$(mtd_get_mac_ascii u-boot-env ethaddr)
		;;
	esac

	[ -n "$lan_mac" ] && ucidef_set_interface_macaddr "lan" $lan_mac
	[ -n "$wan_mac" ] && ucidef_set_interface_macaddr "wan" $wan_mac
	[ -n "$label_mac" ] && ucidef_set_label_macaddr $label_mac
}

board_config_update
board=$(board_name)
ath79_setup_interfaces $board
ath79_setup_macs $board
board_config_flush

exit 0
