From 534a5f99d589cfa6b244b4433c192b6a278a67ff Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Sat, 5 Nov 2022 20:15:40 +0100
Subject: [PATCH] wifi: ath11k: use unique QRTR instance ID

Currently, trying to use AHB + PCI/MHI cards or multiple PCI/MHI cards
will cause a clash in the QRTR instance node ID and prevent the driver
from talking via QMI to the card and thus initializing it with:
[    9.836329] ath11k c000000.wifi: host capability request failed: 1 90
[    9.842047] ath11k c000000.wifi: failed to send qmi host cap: -22

So, in order to allow for this combination of cards, especially AHB + PCI
cards like IPQ8074 + QCN9074 (Used by me and tested on) set the desired
QRTR instance ID offset by calculating a unique one based on PCI domain
and bus ID-s and writing it to bits 7-0 of BHI_ERRDBG2 MHI register by
using the SBL state callback that is added as part of the series.
We also have to make sure that new QRTR offset is added on top of the
default QRTR instance ID-s that are currently used in the driver.

This finally allows using AHB + PCI or multiple PCI cards on the same
system.

Since this is not supported on QCA6390 and like, its limited to QCN9074
which is known to support changing QRTR instance ID.

Before:
root@libreCMC:/# qrtr-lookup
  Service Version Instance Node  Port
     1054       1        0    7     1 <unknown>
       69       1        2    7     3 ATH10k WLAN firmware service

After:
root@libreCMC:/# qrtr-lookup
  Service Version Instance Node  Port
     1054       1        0    7     1 <unknown>
       69       1        2    7     3 ATH10k WLAN firmware service
       15       1        0    8     1 Test service
       69       1        8    8     2 ATH10k WLAN firmware service

Tested-on: IPQ8074 hw2.0 AHB WLAN.HK.2.5.0.1-01208-QCAHKSWPL_SILICONZ-1
Tested-on: QCN9074 hw1.0 PCI WLAN.HK.2.5.0.1-01208-QCAHKSWPL_SILICONZ-1

Signed-off-by: Robert Marko <robimarko@gmail.com>
---
 drivers/net/wireless/ath/ath11k/mhi.c | 49 ++++++++++++++++++---------
 drivers/net/wireless/ath/ath11k/mhi.h |  3 ++
 drivers/net/wireless/ath/ath11k/pci.c |  9 ++++-
 3 files changed, 44 insertions(+), 17 deletions(-)

--- a/drivers/net/wireless/ath/ath11k/mhi.c
+++ b/drivers/net/wireless/ath/ath11k/mhi.c
@@ -294,6 +294,34 @@ static void ath11k_mhi_op_runtime_put(st
 {
 }
 
+static int ath11k_mhi_op_read_reg(struct mhi_controller *mhi_cntrl,
+				  void __iomem *addr,
+				  u32 *out)
+{
+	*out = readl(addr);
+
+	return 0;
+}
+
+static void ath11k_mhi_op_write_reg(struct mhi_controller *mhi_cntrl,
+				    void __iomem *addr,
+				    u32 val)
+{
+	writel(val, addr);
+}
+
+static void ath11k_mhi_qrtr_instance_set(struct mhi_controller *mhi_cntrl)
+{
+	struct ath11k_base *ab = dev_get_drvdata(mhi_cntrl->cntrl_dev);
+
+	if (ab->hw_rev == ATH11K_HW_QCN9074_HW10) {
+		ath11k_mhi_op_write_reg(mhi_cntrl,
+					mhi_cntrl->bhi + BHI_ERRDBG2,
+					FIELD_PREP(QRTR_INSTANCE_MASK,
+					ab->qmi.service_ins_id - ab->hw_params.qmi_service_ins_id));
+	}
+}
+
 static char *ath11k_mhi_op_callback_to_str(enum mhi_callback reason)
 {
 	switch (reason) {
@@ -315,6 +343,8 @@ static char *ath11k_mhi_op_callback_to_s
 		return "MHI_CB_FATAL_ERROR";
 	case MHI_CB_BW_REQ:
 		return "MHI_CB_BW_REQ";
+	case MHI_CB_EE_SBL_MODE:
+		return "MHI_CB_EE_SBL_MODE";
 	default:
 		return "UNKNOWN";
 	}
@@ -336,27 +366,14 @@ static void ath11k_mhi_op_status_cb(stru
 		if (!(test_bit(ATH11K_FLAG_UNREGISTERING, &ab->dev_flags)))
 			queue_work(ab->workqueue_aux, &ab->reset_work);
 		break;
+	case MHI_CB_EE_SBL_MODE:
+		ath11k_mhi_qrtr_instance_set(mhi_cntrl);
+		break;
 	default:
 		break;
 	}
 }
 
-static int ath11k_mhi_op_read_reg(struct mhi_controller *mhi_cntrl,
-				  void __iomem *addr,
-				  u32 *out)
-{
-	*out = readl(addr);
-
-	return 0;
-}
-
-static void ath11k_mhi_op_write_reg(struct mhi_controller *mhi_cntrl,
-				    void __iomem *addr,
-				    u32 val)
-{
-	writel(val, addr);
-}
-
 static int ath11k_mhi_read_addr_from_dt(struct mhi_controller *mhi_ctrl)
 {
 	struct device_node *np;
--- a/drivers/net/wireless/ath/ath11k/mhi.h
+++ b/drivers/net/wireless/ath/ath11k/mhi.h
@@ -16,6 +16,9 @@
 #define MHICTRL					0x38
 #define MHICTRL_RESET_MASK			0x2
 
+#define BHI_ERRDBG2				0x38
+#define QRTR_INSTANCE_MASK			GENMASK(7, 0)
+
 int ath11k_mhi_start(struct ath11k_pci *ar_pci);
 void ath11k_mhi_stop(struct ath11k_pci *ar_pci);
 int ath11k_mhi_register(struct ath11k_pci *ar_pci);
--- a/drivers/net/wireless/ath/ath11k/pci.c
+++ b/drivers/net/wireless/ath/ath11k/pci.c
@@ -370,13 +370,20 @@ static void ath11k_pci_sw_reset(struct a
 static void ath11k_pci_init_qmi_ce_config(struct ath11k_base *ab)
 {
 	struct ath11k_qmi_ce_cfg *cfg = &ab->qmi.ce_cfg;
+	struct ath11k_pci *ab_pci = ath11k_pci_priv(ab);
+	struct pci_bus *bus = ab_pci->pdev->bus;
 
 	cfg->tgt_ce = ab->hw_params.target_ce_config;
 	cfg->tgt_ce_len = ab->hw_params.target_ce_count;
 
 	cfg->svc_to_ce_map = ab->hw_params.svc_to_ce_map;
 	cfg->svc_to_ce_map_len = ab->hw_params.svc_to_ce_map_len;
-	ab->qmi.service_ins_id = ab->hw_params.qmi_service_ins_id;
+
+	if (ab->hw_rev == ATH11K_HW_QCN9074_HW10) {
+		ab->qmi.service_ins_id = ab->hw_params.qmi_service_ins_id +
+		(((pci_domain_nr(bus) & 0xF) << 4) | (bus->number & 0xF));
+	} else
+		ab->qmi.service_ins_id = ab->hw_params.qmi_service_ins_id;
 
 	ath11k_ce_get_shadow_config(ab, &cfg->shadow_reg_v2,
 				    &cfg->shadow_reg_v2_len);
