From 0cf731f9ebb5bf6f252055bebf4463a5c0bd490b Mon Sep 17 00:00:00 2001
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Tue, 23 Aug 2022 14:24:07 +0200
Subject: [PATCH] net: ethernet: mtk_eth_soc: fix hw hash reporting for
 MTK_NETSYS_V2

Properly report hw rx hash for mt7986 chipset accroding to the new dma
descriptor layout.

Fixes: 197c9e9b17b11 ("net: ethernet: mtk_eth_soc: introduce support for mt7986 chipset")
Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Link: https://lore.kernel.org/r/091394ea4e705fbb35f828011d98d0ba33808f69.1661257293.git.lorenzo@kernel.org
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 22 +++++++++++----------
 drivers/net/ethernet/mediatek/mtk_eth_soc.h |  5 +++++
 2 files changed, 17 insertions(+), 10 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -1846,10 +1846,19 @@ static int mtk_poll_rx(struct napi_struc
 		skb->dev = netdev;
 		bytes += skb->len;
 
-		if (MTK_HAS_CAPS(eth->soc->caps, MTK_NETSYS_V2))
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_NETSYS_V2)) {
+			hash = trxd.rxd5 & MTK_RXD5_FOE_ENTRY;
+			if (hash != MTK_RXD5_FOE_ENTRY)
+				skb_set_hash(skb, jhash_1word(hash, 0),
+					     PKT_HASH_TYPE_L4);
 			rxdcsum = &trxd.rxd3;
-		else
+		} else {
+			hash = trxd.rxd4 & MTK_RXD4_FOE_ENTRY;
+			if (hash != MTK_RXD4_FOE_ENTRY)
+				skb_set_hash(skb, jhash_1word(hash, 0),
+					     PKT_HASH_TYPE_L4);
 			rxdcsum = &trxd.rxd4;
+		}
 
 		if (*rxdcsum & eth->soc->txrx.rx_dma_l4_valid)
 			skb->ip_summed = CHECKSUM_UNNECESSARY;
@@ -1857,16 +1866,9 @@ static int mtk_poll_rx(struct napi_struc
 			skb_checksum_none_assert(skb);
 		skb->protocol = eth_type_trans(skb, netdev);
 
-		hash = trxd.rxd4 & MTK_RXD4_FOE_ENTRY;
-		if (hash != MTK_RXD4_FOE_ENTRY) {
-			hash = jhash_1word(hash, 0);
-			skb_set_hash(skb, hash, PKT_HASH_TYPE_L4);
-		}
-
 		reason = FIELD_GET(MTK_RXD4_PPE_CPU_REASON, trxd.rxd4);
 		if (reason == MTK_PPE_CPU_REASON_HIT_UNBIND_RATE_REACHED)
-			mtk_ppe_check_skb(eth->ppe, skb,
-					  trxd.rxd4 & MTK_RXD4_FOE_ENTRY);
+			mtk_ppe_check_skb(eth->ppe, skb, hash);
 
 		if (netdev->features & NETIF_F_HW_VLAN_CTAG_RX) {
 			if (MTK_HAS_CAPS(eth->soc->caps, MTK_NETSYS_V2)) {
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -314,6 +314,11 @@
 #define RX_DMA_L4_VALID_PDMA	BIT(30)		/* when PDMA is used */
 #define RX_DMA_SPECIAL_TAG	BIT(22)
 
+/* PDMA descriptor rxd5 */
+#define MTK_RXD5_FOE_ENTRY	GENMASK(14, 0)
+#define MTK_RXD5_PPE_CPU_REASON	GENMASK(22, 18)
+#define MTK_RXD5_SRC_PORT	GENMASK(29, 26)
+
 #define RX_DMA_GET_SPORT(x)	(((x) >> 19) & 0xf)
 #define RX_DMA_GET_SPORT_V2(x)	(((x) >> 26) & 0x7)
 
