From 0dcbe607cec32ccae23b02a641b8bd6191a328ae Mon Sep 17 00:00:00 2001
Message-Id: <0dcbe607cec32ccae23b02a641b8bd6191a328ae.1662243796.git.lorenzo@kernel.org>
In-Reply-To: <43a21841ce0175d29f23c34a65ceaaf9dd7eb8b7.1662243796.git.lorenzo@kernel.org>
References: <43a21841ce0175d29f23c34a65ceaaf9dd7eb8b7.1662243796.git.lorenzo@kernel.org>
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Tue, 23 Aug 2022 23:09:05 +0200
Subject: [PATCH net-next 2/4] net: ethernet: mtk_eth_soc: move wdma_base
 definitions in mtk register map

This is a preliminary patch to introduce mt7986 wed support.

Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 16 ++++++++++------
 drivers/net/ethernet/mediatek/mtk_eth_soc.h |  4 +---
 2 files changed, 11 insertions(+), 9 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -75,6 +75,10 @@ static const struct mtk_reg_map mtk_reg_
 	.gdm1_cnt		= 0x2400,
 	.gdma_to_ppe0		= 0x4444,
 	.ppe_base		= 0x0c00,
+	.wdma_base = {
+		[0]		= 0x2800,
+		[1]		= 0x2c00,
+	},
 };
 
 static const struct mtk_reg_map mt7628_reg_map = {
@@ -130,6 +134,10 @@ static const struct mtk_reg_map mt7986_r
 	.gdm1_cnt		= 0x1c00,
 	.gdma_to_ppe0		= 0x3333,
 	.ppe_base		= 0x2000,
+	.wdma_base = {
+		[0]		= 0x4800,
+		[1]		= 0x4c00,
+	},
 };
 
 /* strings used by ethtool */
@@ -3966,16 +3974,12 @@ static int mtk_probe(struct platform_dev
 	for (i = 0;; i++) {
 		struct device_node *np = of_parse_phandle(pdev->dev.of_node,
 							  "mediatek,wed", i);
-		static const u32 wdma_regs[] = {
-			MTK_WDMA0_BASE,
-			MTK_WDMA1_BASE
-		};
 		void __iomem *wdma;
 
-		if (!np || i >= ARRAY_SIZE(wdma_regs))
+		if (!np || i >= ARRAY_SIZE(eth->soc->reg_map->wdma_base))
 			break;
 
-		wdma = eth->base + wdma_regs[i];
+		wdma = eth->base + eth->soc->reg_map->wdma_base[i];
 		mtk_wed_add_hw(np, eth, wdma, i);
 	}
 
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -268,9 +268,6 @@
 #define TX_DMA_FPORT_MASK_V2	0xf
 #define TX_DMA_SWC_V2		BIT(30)
 
-#define MTK_WDMA0_BASE		0x2800
-#define MTK_WDMA1_BASE		0x2c00
-
 /* QDMA descriptor txd4 */
 #define TX_DMA_CHKSUM		(0x7 << 29)
 #define TX_DMA_TSO		BIT(28)
@@ -954,6 +951,7 @@ struct mtk_reg_map {
 	u32	gdm1_cnt;
 	u32	gdma_to_ppe0;
 	u32	ppe_base;
+	u32	wdma_base[2];
 };
 
 /* struct mtk_eth_data -	This is the structure holding all differences
