From 71d927494463c4f016d828e1134da26b7e961af5 Mon Sep 17 00:00:00 2001
From: "Russell King (Oracle)" <rmk+kernel@armlinux.org.uk>
Date: Tue, 16 Nov 2021 10:06:53 +0000
Subject: [PATCH] net: mtk_eth_soc: drop use of phylink_helper_basex_speed()

Now that we have a better method to select SFP interface modes, we
no longer need to use phylink_helper_basex_speed() in a driver's
validation function, and we can also get rid of our hack to indicate
both 1000base-X and 2500base-X if the comphy is present to make that
work. Remove this hack and use of phylink_helper_basex_speed().

Signed-off-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 8 ++------
 1 file changed, 2 insertions(+), 6 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -578,8 +578,9 @@ static void mtk_validate(struct phylink_
 		phylink_set(mask, 1000baseT_Full);
 		break;
 	case PHY_INTERFACE_MODE_1000BASEX:
-	case PHY_INTERFACE_MODE_2500BASEX:
 		phylink_set(mask, 1000baseX_Full);
+		break;
+	case PHY_INTERFACE_MODE_2500BASEX:
 		phylink_set(mask, 2500baseX_Full);
 		break;
 	case PHY_INTERFACE_MODE_GMII:
@@ -609,11 +610,6 @@ static void mtk_validate(struct phylink_
 
 	linkmode_and(supported, supported, mask);
 	linkmode_and(state->advertising, state->advertising, mask);
-
-	/* We can only operate at 2500BaseX or 1000BaseX. If requested
-	 * to advertise both, only report advertising at 2500BaseX.
-	 */
-	phylink_helper_basex_speed(state);
 }
 
 static const struct phylink_mac_ops mtk_phylink_ops = {
