#!/bin/sh /etc/rc.common
# SPDX-License-Identifier: GPL-2.0-or-later

START=11

boot() {
	. /lib/functions.sh
	/usr/sbin/nu801 "$(board_name)"

	# Because this is a userspace driver, we need to trigger diag.sh after
	# we start the driver, but before boot is complete so we blink.
	. /etc/diag.sh
	set_state preinit_regular
}
