// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "compex,wpj344-16m", "qca,ar9344";
	model = "Compex WPJ344 (16MB flash)";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	leds {
		compatible = "gpio-leds";

		led_status: status {
			label = "green:status";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		sig1 {
			label = "red:sig1";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		sig2 {
			label = "yellow:sig2";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};

		sig3 {
			label = "green:sig3";
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};

		sig4 {
			label = "green:sig4";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x030000>;
				read-only;
			};

			partition@30000 {
				label = "firmware";
				reg = <0x030000 0xfc0000>;
				compatible = "denx,uimage";
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&usb {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&pcie {
	status = "okay";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "rgmii";

		qca,ar8327-initvals = <
			0x04 0x07600000 /* PORT0 PAD MODE CTRL */
			0x10 0x80000080 /* POWER_ON_STRAP */
			0x50 0x00000000 /* LED_CTRL0 */
			0x54 0xc737c737 /* LED_CTRL1 */
			0x58 0x00000000 /* LED_CTRL2 */
			0x5c 0x00c30c00 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x06000000 0x00000101 0x00001616>;

	nvmem-cells = <&macaddr_uboot_2e010>;
	nvmem-cell-names = "mac-address";

	phy-mode = "rgmii";
	phy-handle = <&phy0>;
};

&uboot {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_uboot_2e010: macaddr@2e010 {
		reg = <0x2e010 0x6>;
	};
};
