From 281f7a6c1a33fffcde32001bacbb4f672140fbf9 Mon Sep 17 00:00:00 2001
From: Michael Walle <michael@walle.cc>
Date: Wed, 8 Mar 2023 09:20:21 +0100
Subject: [PATCH] mtd: core: prepare mtd_otp_nvmem_add() to handle
 -EPROBE_DEFER

NVMEM soon will get the ability for nvmem layouts and these might
not be ready when nvmem_register() is called and thus it might
return -EPROBE_DEFER. Don't print the error message in this case.

Signed-off-by: Michael Walle <michael@walle.cc>
Signed-off-by: Miquel Raynal <miquel.raynal@bootlin.com>
Link: https://lore.kernel.org/linux-mtd/20230308082021.870459-4-michael@walle.cc
---
 drivers/mtd/mtdcore.c | 7 +++----
 1 file changed, 3 insertions(+), 4 deletions(-)

--- a/drivers/mtd/mtdcore.c
+++ b/drivers/mtd/mtdcore.c
@@ -960,8 +960,8 @@ static int mtd_otp_nvmem_add(struct mtd_
 			nvmem = mtd_otp_nvmem_register(mtd, "user-otp", size,
 						       mtd_nvmem_user_otp_reg_read);
 			if (IS_ERR(nvmem)) {
-				dev_err(dev, "Failed to register OTP NVMEM device\n");
-				return PTR_ERR(nvmem);
+				err = PTR_ERR(nvmem);
+				goto err;
 			}
 			mtd->otp_user_nvmem = nvmem;
 		}
@@ -978,7 +978,6 @@ static int mtd_otp_nvmem_add(struct mtd_
 			nvmem = mtd_otp_nvmem_register(mtd, "factory-otp", size,
 						       mtd_nvmem_fact_otp_reg_read);
 			if (IS_ERR(nvmem)) {
-				dev_err(dev, "Failed to register OTP NVMEM device\n");
 				err = PTR_ERR(nvmem);
 				goto err;
 			}
@@ -991,7 +990,7 @@ static int mtd_otp_nvmem_add(struct mtd_
 err:
 	if (mtd->otp_user_nvmem)
 		nvmem_unregister(mtd->otp_user_nvmem);
-	return err;
+	return dev_err_probe(dev, err, "Failed to register OTP NVMEM device\n");
 }
 
 /**
