From b804f765485109f9644cc05d1e8fc79ca6c6e4aa Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Wed, 19 Jul 2023 01:39:36 +0100
Subject: [PATCH 094/250] net: ethernet: mtk_eth_soc: always
 mtk_get_ib1_pkt_type

entries and bind debugfs files would display wrong data on NETSYS_V2 and
later because instead of using mtk_get_ib1_pkt_type the driver would use
MTK_FOE_IB1_PACKET_TYPE which corresponds to NETSYS_V1(.x) SoCs.
Use mtk_get_ib1_pkt_type so entries and bind records display correctly.

Fixes: 03a3180e5c09e ("net: ethernet: mtk_eth_soc: introduce flow offloading support for mt7986")
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Acked-by: Lorenzo Bianconi <lorenzo@kernel.org>
Link: https://lore.kernel.org/r/c0ae03d0182f4d27b874cbdf0059bc972c317f3c.1689727134.git.daniel@makrotopia.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/mediatek/mtk_ppe_debugfs.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/mediatek/mtk_ppe_debugfs.c
+++ b/drivers/net/ethernet/mediatek/mtk_ppe_debugfs.c
@@ -98,7 +98,7 @@ mtk_ppe_debugfs_foe_show(struct seq_file
 
 		acct = mtk_foe_entry_get_mib(ppe, i, NULL);
 
-		type = FIELD_GET(MTK_FOE_IB1_PACKET_TYPE, entry->ib1);
+		type = mtk_get_ib1_pkt_type(ppe->eth, entry->ib1);
 		seq_printf(m, "%05x %s %7s", i,
 			   mtk_foe_entry_state_str(state),
 			   mtk_foe_pkt_type_str(type));
