From 58344a3b85f1bd5ffddfc2c11f6f2bf688b5f990 Mon Sep 17 00:00:00 2001
From: "Russell King (Oracle)" <rmk+kernel@armlinux.org.uk>
Date: Mon, 11 Apr 2022 10:46:12 +0100
Subject: [PATCH 04/13] net: dsa: mt7530: drop use of
 phylink_helper_basex_speed()
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Now that we have a better method to select SFP interface modes, we
no longer need to use phylink_helper_basex_speed() in a driver's
validation function.

Tested-by: Marek Behún <kabel@kernel.org>
Signed-off-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/dsa/mt7530.c | 5 -----
 1 file changed, 5 deletions(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -3009,11 +3009,6 @@ mt753x_phylink_validate(struct dsa_switc
 
 	linkmode_and(supported, supported, mask);
 	linkmode_and(state->advertising, state->advertising, mask);
-
-	/* We can only operate at 2500BaseX or 1000BaseX.  If requested
-	 * to advertise both, only report advertising at 2500BaseX.
-	 */
-	phylink_helper_basex_speed(state);
 }
 
 static int
