--- a/drivers/net/wireless/ath/ath9k/debug.c
+++ b/drivers/net/wireless/ath/ath9k/debug.c
@@ -1374,6 +1374,53 @@ void ath9k_deinit_debug(struct ath_softc
 	ath9k_cmn_spectral_deinit_debug(&sc->spec_priv);
 }
 
+static ssize_t read_file_eeprom(struct file *file, char __user *user_buf,
+			     size_t count, loff_t *ppos)
+{
+	struct ath_softc *sc = file->private_data;
+	struct ath_hw *ah = sc->sc_ah;
+	struct ath_common *common = ath9k_hw_common(ah);
+	int bytes = 0;
+	int pos = *ppos;
+	int size = 4096;
+	u16 val;
+	int i;
+
+	if (AR_SREV_9300_20_OR_LATER(ah))
+		size = 16384;
+
+	if (*ppos < 0)
+		return -EINVAL;
+
+	if (count > size - *ppos)
+		count = size - *ppos;
+
+	for (i = *ppos / 2; count > 0; count -= bytes, *ppos += bytes, i++) {
+		void *from = &val;
+
+		if (!common->bus_ops->eeprom_read(common, i, &val))
+			val = 0xffff;
+
+		if (*ppos % 2) {
+			from++;
+			bytes = 1;
+		} else if (count == 1) {
+			bytes = 1;
+		} else {
+			bytes = 2;
+		}
+		copy_to_user(user_buf, from, bytes);
+		user_buf += bytes;
+	}
+	return *ppos - pos;
+}
+
+static const struct file_operations fops_eeprom = {
+	.read = read_file_eeprom,
+	.open = simple_open,
+	.owner = THIS_MODULE
+};
+
 int ath9k_init_debug(struct ath_hw *ah)
 {
 	struct ath_common *common = ath9k_hw_common(ah);
@@ -1393,6 +1440,8 @@ int ath9k_init_debug(struct ath_hw *ah)
 	ath9k_tx99_init_debug(sc);
 	ath9k_cmn_spectral_init_debug(&sc->spec_priv, sc->debug.debugfs_phy);
 
+	debugfs_create_file("eeprom", S_IRUSR, sc->debug.debugfs_phy, sc,
+			    &fops_eeprom);
 	debugfs_create_devm_seqfile(sc->dev, "dma", sc->debug.debugfs_phy,
 				    read_file_dma);
 	debugfs_create_devm_seqfile(sc->dev, "interrupt", sc->debug.debugfs_phy,
