From 43ebc7c1b3ed8198b9acf3019eca16e722f7331c Mon Sep 17 00:00:00 2001
From: Ding Tao <miyatsu@qq.com>
Date: Fri, 26 Oct 2018 11:50:28 +0000
Subject: [PATCH] arm64: dts: marvell: armada-37xx: Enable emmc on espressobin

The ESPRESSObin board has a emmc interface available on U11: declare it
and let the bootloader enable it if the emmc is present.

[gregory.clement@bootlin.com: disable the emmc by default]
Signed-off-by: Ding Tao <miyatsu@qq.com>
Signed-off-by: Gregory CLEMENT <gregory.clement@bootlin.com>
---
 .../dts/marvell/armada-3720-espressobin.dts   | 22 +++++++++++++++++++
 1 file changed, 22 insertions(+)

--- a/arch/arm64/boot/dts/marvell/armada-3720-espressobin.dts
+++ b/arch/arm64/boot/dts/marvell/armada-3720-espressobin.dts
@@ -100,9 +100,31 @@
 	cd-gpios = <&gpionb 3 GPIO_ACTIVE_LOW>;
 	marvell,pad-type = "sd";
 	vqmmc-supply = <&vcc_sd_reg1>;
+
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio_pins>;
 	status = "okay";
 };
 
+/* U11 */
+&sdhci0 {
+	non-removable;
+	bus-width = <8>;
+	mmc-ddr-1_8v;
+	mmc-hs400-1_8v;
+	marvell,xenon-emmc;
+	marvell,xenon-tun-count = <9>;
+	marvell,pad-type = "fixed-1-8v";
+
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc_pins>;
+/*
+ * This eMMC is not populated on all boards, so disable it by
+ * default and let the bootloader enable it, if it is present
+ */
+	status = "disabled";
+};
+
 &spi0 {
 	status = "okay";
 
