From 0720be5371c806c1b89936984a321248fa739bea Mon Sep 17 00:00:00 2001
From: David Bauer <mail@david-bauer.net>
Date: Fri, 10 Jul 2020 15:57:46 +0200
Subject: [PATCH] rockchip: rk3328: Add support for FriendlyARM NanoPi R2S

This adds support for the NanoPi R2S from FriendlyARM.

Rockchip RK3328 SoC
1GB DDR4 RAM
Gigabit Ethernet (WAN)
Gigabit Ethernet (USB3) (LAN)
USB 2.0 Host Port
MicroSD slot
Reset button
WAN - LAN - SYS LED

Signed-off-by: David Bauer <mail@david-bauer.net>
---
 arch/arm64/boot/dts/rockchip/Makefile         |   1 +
 .../boot/dts/rockchip/rk3328-nanopi-r2s.dts   | 368 ++++++++++++++++++
 2 files changed, 369 insertions(+)
 create mode 100644 arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts

--- a/arch/arm64/boot/dts/rockchip/Makefile
+++ b/arch/arm64/boot/dts/rockchip/Makefile
@@ -7,6 +7,7 @@ dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3368-or
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3368-px5-evb.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3368-r88.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-evb.dtb
+dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3328-nanopi-r2s.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-firefly.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-gru-kevin.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3399-puma-haikou.dtb
--- /dev/null
+++ b/arch/arm64/boot/dts/rockchip/rk3328-nanopi-r2s.dts
@@ -0,0 +1,368 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Copyright (c) 2020 David Bauer <mail@david-bauer.net>
+ */
+
+/dts-v1/;
+
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/gpio/gpio.h>
+#include "rk3328.dtsi"
+
+/ {
+	model = "FriendlyElec NanoPi R2S";
+	compatible = "friendlyarm,nanopi-r2s", "rockchip,rk3328";
+
+	chosen {
+		stdout-path = "serial2:1500000n8";
+	};
+
+	gmac_clk: gmac-clock {
+		compatible = "fixed-clock";
+		clock-frequency = <125000000>;
+		clock-output-names = "gmac_clk";
+		#clock-cells = <0>;
+	};
+
+	keys {
+		compatible = "gpio-keys";
+		pinctrl-0 = <&reset_button_pin>;
+		pinctrl-names = "default";
+
+		reset {
+			label = "reset";
+			gpios = <&gpio0 RK_PA0 GPIO_ACTIVE_LOW>;
+			linux,code = <KEY_RESTART>;
+			debounce-interval = <50>;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+		pinctrl-0 = <&lan_led_pin>,  <&sys_led_pin>, <&wan_led_pin>;
+		pinctrl-names = "default";
+
+		lan_led: led-0 {
+			gpios = <&gpio2 RK_PB7 GPIO_ACTIVE_HIGH>;
+			label = "nanopi-r2s:green:lan";
+		};
+
+		sys_led: led-1 {
+			gpios = <&gpio0 RK_PA2 GPIO_ACTIVE_HIGH>;
+			label = "nanopi-r2s:red:sys";
+		};
+
+		wan_led: led-2 {
+			gpios = <&gpio2 RK_PC2 GPIO_ACTIVE_HIGH>;
+			label = "nanopi-r2s:green:wan";
+		};
+	};
+
+	vcc_io_sdio: sdmmcio-regulator {
+		compatible = "regulator-gpio";
+		enable-active-high;
+		gpios = <&gpio1 RK_PD4 GPIO_ACTIVE_HIGH>;
+		pinctrl-0 = <&sdio_vcc_pin>;
+		pinctrl-names = "default";
+		regulator-name = "vcc_io_sdio";
+		regulator-always-on;
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-settling-time-us = <5000>;
+		regulator-type = "voltage";
+		startup-delay-us = <2000>;
+		states = <1800000 0x1
+			  3300000 0x0>;
+		vin-supply = <&vcc_io_33>;
+	};
+
+	vcc_sd: sdmmc-regulator {
+		compatible = "regulator-fixed";
+		gpio = <&gpio0 RK_PD6 GPIO_ACTIVE_LOW>;
+		pinctrl-0 = <&sdmmc0m1_gpio>;
+		pinctrl-names = "default";
+		regulator-name = "vcc_sd";
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vcc_io_33>;
+	};
+
+	vdd_5v: vdd-5v {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd_5v";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu1 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu2 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&cpu3 {
+	cpu-supply = <&vdd_arm>;
+};
+
+&gmac2io {
+	assigned-clocks = <&cru SCLK_MAC2IO>, <&cru SCLK_MAC2IO_EXT>;
+	assigned-clock-parents = <&gmac_clk>, <&gmac_clk>;
+	clock_in_out = "input";
+	phy-handle = <&rtl8211e>;
+	phy-mode = "rgmii";
+	phy-supply = <&vcc_io_33>;
+	pinctrl-0 = <&rgmiim1_pins>;
+	pinctrl-names = "default";
+	rx_delay = <0x18>;
+	snps,aal;
+	tx_delay = <0x24>;
+	status = "okay";
+
+	mdio {
+		compatible = "snps,dwmac-mdio";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		rtl8211e: ethernet-phy@1 {
+			reg = <1>;
+			pinctrl-0 = <&eth_phy_reset_pin>;
+			pinctrl-names = "default";
+			reset-assert-us = <10000>;
+			reset-deassert-us = <50000>;
+			reset-gpios = <&gpio1 RK_PC2 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&i2c1 {
+	status = "okay";
+
+	rk805: pmic@18 {
+		compatible = "rockchip,rk805";
+		reg = <0x18>;
+		interrupt-parent = <&gpio1>;
+		interrupts = <24 IRQ_TYPE_LEVEL_LOW>;
+		#clock-cells = <1>;
+		clock-output-names = "xin32k", "rk805-clkout2";
+		gpio-controller;
+		#gpio-cells = <2>;
+		pinctrl-0 = <&pmic_int_l>;
+		pinctrl-names = "default";
+		rockchip,system-power-controller;
+		wakeup-source;
+
+		vcc1-supply = <&vdd_5v>;
+		vcc2-supply = <&vdd_5v>;
+		vcc3-supply = <&vdd_5v>;
+		vcc4-supply = <&vdd_5v>;
+		vcc5-supply = <&vcc_io_33>;
+		vcc6-supply = <&vdd_5v>;
+
+		regulators {
+			vdd_log: DCDC_REG1 {
+				regulator-name = "vdd_log";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <712500>;
+				regulator-max-microvolt = <1450000>;
+				regulator-ramp-delay = <12500>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1000000>;
+				};
+			};
+
+			vdd_arm: DCDC_REG2 {
+				regulator-name = "vdd_arm";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <712500>;
+				regulator-max-microvolt = <1450000>;
+				regulator-ramp-delay = <12500>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <950000>;
+				};
+			};
+
+			vcc_ddr: DCDC_REG3 {
+				regulator-name = "vcc_ddr";
+				regulator-always-on;
+				regulator-boot-on;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+				};
+			};
+
+			vcc_io_33: DCDC_REG4 {
+				regulator-name = "vcc_io_33";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3300000>;
+				};
+			};
+
+			vcc_18: LDO_REG1 {
+				regulator-name = "vcc_18";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vcc18_emmc: LDO_REG2 {
+				regulator-name = "vcc18_emmc";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vdd_10: LDO_REG3 {
+				regulator-name = "vdd_10";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1000000>;
+				regulator-max-microvolt = <1000000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1000000>;
+				};
+			};
+		};
+	};
+};
+
+&io_domains {
+	pmuio-supply = <&vcc_io_33>;
+	vccio1-supply = <&vcc_io_33>;
+	vccio2-supply = <&vcc18_emmc>;
+	vccio3-supply = <&vcc_io_sdio>;
+	vccio4-supply = <&vcc_18>;
+	vccio5-supply = <&vcc_io_33>;
+	vccio6-supply = <&vcc_io_33>;
+	status = "okay";
+};
+
+&pinctrl {
+	button {
+		reset_button_pin: reset-button-pin {
+			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	ethernet-phy {
+		eth_phy_reset_pin: eth-phy-reset-pin {
+			rockchip,pins = <1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+	};
+
+	leds {
+		lan_led_pin: lan-led-pin {
+			rockchip,pins = <2 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		sys_led_pin: sys-led-pin {
+			rockchip,pins = <0 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		wan_led_pin: wan-led-pin {
+			rockchip,pins = <2 RK_PC2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	pmic {
+		pmic_int_l: pmic-int-l {
+			rockchip,pins = <1 RK_PD0 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	sd {
+		sdio_vcc_pin: sdio-vcc-pin {
+			rockchip,pins = <1 RK_PD4 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+};
+
+&pwm2 {
+	status = "okay";
+};
+
+&sdmmc {
+	bus-width = <4>;
+	cap-sd-highspeed;
+	disable-wp;
+	pinctrl-0 = <&sdmmc0_clk>, <&sdmmc0_cmd>, <&sdmmc0_dectn>, <&sdmmc0_bus4>;
+	pinctrl-names = "default";
+	sd-uhs-sdr12;
+	sd-uhs-sdr25;
+	sd-uhs-sdr50;
+	sd-uhs-sdr104;
+	vmmc-supply = <&vcc_sd>;
+	vqmmc-supply = <&vcc_io_sdio>;
+	status = "okay";
+};
+
+&tsadc {
+	rockchip,hw-tshut-mode = <0>;
+	rockchip,hw-tshut-polarity = <0>;
+	status = "okay";
+};
+
+&u2phy {
+	status = "okay";
+};
+
+&u2phy_host {
+	status = "okay";
+};
+
+&u2phy_otg {
+	status = "okay";
+};
+
+&uart2 {
+	status = "okay";
+};
+
+&usb20_otg {
+	status = "okay";
+	dr_mode = "host";
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
