From: André Valentin <avalentin@marcant.net>
Subject: linux/mtd: add id for mx25u3235f needed by ZyXEL NBG6817

Signed-off-by: André Valentin <avalentin@marcant.net>
---
 drivers/mtd/spi-nor/spi-nor.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -1022,6 +1022,7 @@ static const struct flash_info spi_nor_i
 	{ "mx25l3205d",  INFO(0xc22016, 0, 64 * 1024,  64, SECT_4K) },
 	{ "mx25l3255e",  INFO(0xc29e16, 0, 64 * 1024,  64, SECT_4K) },
 	{ "mx25l6405d",  INFO(0xc22017, 0, 64 * 1024, 128, SECT_4K) },
+	{ "mx25u3235f",	 INFO(0xc22536, 0, 64 * 1024, 64, 0) },
 	{ "mx25u2033e",  INFO(0xc22532, 0, 64 * 1024,   4, SECT_4K) },
 	{ "mx25u4035",   INFO(0xc22533, 0, 64 * 1024,   8, SECT_4K) },
 	{ "mx25u8035",   INFO(0xc22534, 0, 64 * 1024,  16, SECT_4K) },
