// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "jjPlus JWAP230";
	compatible = "jjplus,jwap230", "qca,qca9558";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	leds {
		compatible = "gpio-leds";

		led_power: led-0 {
			label = "green:power";
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		led-1 {
			color = <LED_COLOR_ID_GREEN>;
			function-enumerator = <0>;
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		led-2 {
			color = <LED_COLOR_ID_GREEN>;
			function-enumerator = <1>;
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};
	};
};

&pcie0 {
	status = "okay";
};

&pcie1 {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x050000 0xfa0000>;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_art_lan: macaddr@0 {
					reg = <0x0 0x6>;
				};

				macaddr_art_wan: macaddr@6 {
					reg = <0x6 0x6>;
				};

				calibration_art_wlan: calibration@1000 {
					reg = <0x1000 0x440>;
				};
			};
		};
	};
};

&mdio0 {
	status = "okay";

	switch {
		compatible = "qca,ar8327";
		reg = <0>;

		qca,ar8327-initvals = <
			0x04 0x07600000 /* PORT0 PAD MODE CTRL */
			0x58 0xffb7ffb7 /* LED_CTRL2 */
			0x5c 0x03ffff00 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x0c 0x00080080 /* PORT6 PAD MODE CTRL */
			0x94 0x0000007e /* PORT6_STATUS */
		>;
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_wan>;
	nvmem-cell-names = "mac-address";

	pll-data = <0xae000000 0x80000101 0x80001313>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};

	gmac_config: gmac-config {
		device = <&gmac>;

		rxdv-delay = <3>;
		rxd-delay = <3>;
		txen-delay = <0>;
		txd-delay = <0>;
		rgmii-enabled = <1>;
	};
};

&eth1 {
	status = "okay";

	nvmem-cells = <&macaddr_art_lan>;
	nvmem-cell-names = "mac-address";

	pll-data = <0x03000101 0x00000101 0x00001313>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&wmac {
	status = "okay";
	nvmem-cells = <&calibration_art_wlan>;
	nvmem-cell-names = "calibration";
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb1 {
	status = "okay";
};
