// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "enterasys,ws-ap3705i", "qca,ar9344";
	model = "Enterasys WS-AP3705i";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_red;
		label-mac-device = &eth0;
	};

	mtd-concat {
		compatible = "mtd-concat";
		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x0 0x1dd0000>;
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&enable_gpio_11 &enable_gpio_16>;

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led_power_red: power_red {
			label = "red:power";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		lan_blue {
			label = "blue:lan";
			gpios = <&gpio 19 GPIO_ACTIVE_HIGH>;
		};

		lan_green {
			label = "green:lan";
			gpios = <&gpio 20 GPIO_ACTIVE_HIGH>;
		};

		radio2 {
			label = "green:radio2";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		radio1 {
			label = "green:radio1";
			gpios = <&ath9k 0 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&pinmux {
	enable_gpio_16: pinmux_enable_gpio_16 {
		pinctrl-single,bits = <0x10 0x0 0x000000ff>;
	};

	enable_gpio_11: pinmux_enable_gpio_11 {
		pinctrl-single,bits = <0x8 0x0 0xff000000>;
	};
};

&wmac {
	status = "okay";
	qca,no-eeprom;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot-bak";
				reg = <0x0 0x80000>;
				read-only;
			};

			partition@80000 {
				label = "u-boot-env0";
				reg = <0x80000 0x10000>;
				read-only;
			};

			partition@90000 {
				label = "u-boot-env1";
				reg = <0x90000 0x10000>;
				read-only;
			};

			partition@a0000 {
				label = "u-boot";
				reg = <0xa0000 0x80000>;
				read-only;
			};

			partition@120000 {
				label = "calibrate";
				reg = <0x120000 0x10000>;
				read-only;
			};

			partition@130000 {
				label = "nvram";
				reg = <0x130000 0x100000>;
				read-only;
			};

			fwconcat0: partition@230000 {
				label = "fwconcat0";
				reg = <0x230000 0xdd0000>;
			};
		};
	};

	flash@1 {
		compatible = "jedec,spi-nor";
		reg = <1>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			fwconcat1: partition@0 {
				label = "fwconcat1";
				reg = <0x0 0x1000000>;
			};
		};
	};
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		compatible = "pci168c,0033";
		reg = <0x0000 0 0 0 0>;
		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x1e000000 0x08000101 0x08001313>;

	phy-mode = "rgmii";
	phy-handle = <&phy0>;

	gmac-config {
		device = <&gmac>;
		rgmii-gmac0 = <1>;
		rxd-delay = <0>;
		rxdv-delay = <0>;
		txen-delay = <0>;
		txd-delay = <0>;
	};
};
