From fdbbe242c15a8f2cd0e3ad8a56cd0a447b771d0d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Tue, 30 Nov 2021 18:29:13 +0100
Subject: [PATCH] PCI: aardvark: Disable common PHY when unbinding driver
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Disable the PCIe PHY when unbinding driver. This should save some power.

Link: https://lore.kernel.org/r/20211130172913.9727-12-kabel@kernel.org
Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
Signed-off-by: Lorenzo Pieralisi <lorenzo.pieralisi@arm.com>
---
 drivers/pci/controller/pci-aardvark.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -1745,6 +1745,9 @@ static int advk_pcie_remove(struct platf
 	for (i = 0; i < OB_WIN_COUNT; i++)
 		advk_pcie_disable_ob_win(pcie, i);
 
+	/* Disable phy */
+	advk_pcie_disable_phy(pcie);
+
 	return 0;
 }
 
