From 735a4ac9782b96fbe1543c578aa8334364f21abd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Fri, 2 Apr 2021 14:05:24 +0200
Subject: [PATCH] PCI: aardvark: Enable MSI-X support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

According to PCI 3.0 specification, sending both MSI and MSI-X interrupts
is done by DWORD memory write operation to doorbell message address. The
write operation for MSI has zero upper 16 bits and the MSI interrupt number
in the lower 16 bits, while the write operation for MSI-X contains a 32-bit
value from MSI-X table.

Since the driver only uses interrupt numbers from range 0..31, the upper
16 bits of the DWORD memory write operation to doorbell message address
are zero even for MSI-X interrupts. Thus we can enable MSI-X interrupts.

Testing proves that kernel can correctly receive MSI-X interrupts from PCIe
cards which supports both MSI and MSI-X interrupts.

Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/pci/controller/pci-aardvark.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -1346,7 +1346,7 @@ static struct irq_chip advk_msi_irq_chip
 
 static struct msi_domain_info advk_msi_domain_info = {
 	.flags	= MSI_FLAG_USE_DEF_DOM_OPS | MSI_FLAG_USE_DEF_CHIP_OPS |
-		  MSI_FLAG_MULTI_PCI_MSI,
+		  MSI_FLAG_MULTI_PCI_MSI | MSI_FLAG_PCI_MSIX,
 	.chip	= &advk_msi_irq_chip,
 };
 
