// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "white:system";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan {
			label = "white:wlan";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		lan {
			label = "white:lan";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		usb {
			label = "white:usb";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port1>, <&hub_port0>;
			linux,default-trigger = "usbport";
		};

		qss {
			label = "white:qss";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wifi {
			label = "WiFi button";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};

	reg_usb0_vbus: regulator {
		compatible = "regulator-fixed";
		regulator-name = "usb_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio 21 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	reg_usb1_vbus: regulator {
		compatible = "regulator-fixed";
		regulator-name = "usb_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio 22 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;

		qca,ar8327-initvals = <
			0x04 0x00080080 /* PORT0 PAD MODE CTRL */
			0x0c 0x07600000 /* PORT6 PAD MODE CTRL */
			0x50 0xc737c737 /* LED_CTRL0 */
			0x54 0x00000000 /* LED_CTRL1 */
			0x58 0x00000000 /* LED_CTRL2 */
			0x5c 0x0030c300 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x94 0x0000007e /* PORT6 STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy0>;
	pll-data = <0x56000000 0x00000101 0x00001616>;

	gmac-config {
		device = <&gmac>;
		rgmii-enabled = <1>;
	};
};

&eth1 {
	status = "okay";

	pll-data = <0x03000101 0x00000101 0x00001616>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&wmac {
	status = "okay";
};

&pcie1 {
	status = "okay";
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	dr_mode = "host";
	vbus-supply = <&reg_usb0_vbus>;
	status = "okay";

	hub_port0: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&usb_phy1 {
	status = "okay";
};

&usb1 {
	#address-cells = <1>;
	#size-cells = <0>;
	dr_mode = "host";
	vbus-supply = <&reg_usb1_vbus>;
	status = "okay";

	hub_port1: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};
