From 43f3f187e6f62ca40802afe39495c8a3e20b4bfa Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Mon, 10 Jan 2022 01:50:50 +0100
Subject: [PATCH] PCI: aardvark: Replace custom PCIE_CORE_INT_* macros with
 PCI_INTERRUPT_*
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Header file linux/pci.h defines enum pci_interrupt_pin with corresponding
PCI_INTERRUPT_* values.

Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/pci/controller/pci-aardvark.c | 6 +-----
 1 file changed, 1 insertion(+), 5 deletions(-)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -37,10 +37,6 @@
 #define     PCIE_CORE_ERR_CAPCTL_ECRC_CHK_TX_EN			BIT(6)
 #define     PCIE_CORE_ERR_CAPCTL_ECRC_CHCK			BIT(7)
 #define     PCIE_CORE_ERR_CAPCTL_ECRC_CHCK_RCV			BIT(8)
-#define     PCIE_CORE_INT_A_ASSERT_ENABLE			1
-#define     PCIE_CORE_INT_B_ASSERT_ENABLE			2
-#define     PCIE_CORE_INT_C_ASSERT_ENABLE			3
-#define     PCIE_CORE_INT_D_ASSERT_ENABLE			4
 /* PIO registers base address and register offsets */
 #define PIO_BASE_ADDR				0x4000
 #define PIO_CTRL				(PIO_BASE_ADDR + 0x0)
@@ -968,7 +964,7 @@ static int advk_sw_pci_bridge_init(struc
 	bridge->conf.pref_mem_limit = cpu_to_le16(PCI_PREF_RANGE_TYPE_64);
 
 	/* Support interrupt A for MSI feature */
-	bridge->conf.intpin = PCIE_CORE_INT_A_ASSERT_ENABLE;
+	bridge->conf.intpin = PCI_INTERRUPT_INTA;
 
 	/* Aardvark HW provides PCIe Capability structure in version 2 */
 	bridge->pcie_conf.cap = cpu_to_le16(2);
