From f477d1c8bdbef4f400718238e350f16f521d2a3e Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Thu, 14 Oct 2021 00:39:17 +0200
Subject: net: dsa: qca8k: add support for QCA8328

QCA8328 switch is the bigger brother of the qca8327. Same regs different
chip. Change the function to set the correct pin layout and introduce a
new match_data to differentiate the 2 switch as they have the same ID
and their internal PHY have the same ID.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/dsa/qca8k.c | 19 ++++++++++++++++---
 drivers/net/dsa/qca8k.h |  1 +
 2 files changed, 17 insertions(+), 3 deletions(-)

--- a/drivers/net/dsa/qca8k.c
+++ b/drivers/net/dsa/qca8k.c
@@ -935,6 +935,7 @@ static int
 qca8k_setup_of_pws_reg(struct qca8k_priv *priv)
 {
 	struct device_node *node = priv->dev->of_node;
+	const struct qca8k_match_data *data;
 	u32 val = 0;
 	int ret;
 
@@ -943,8 +944,14 @@ qca8k_setup_of_pws_reg(struct qca8k_priv
 	 * Should be applied by default but we set this just to make sure.
 	 */
 	if (priv->switch_id == QCA8K_ID_QCA8327) {
+		data = of_device_get_match_data(priv->dev);
+
+		/* Set the correct package of 148 pin for QCA8327 */
+		if (data->reduced_package)
+			val |= QCA8327_PWS_PACKAGE148_EN;
+
 		ret = qca8k_rmw(priv, QCA8K_REG_PWS, QCA8327_PWS_PACKAGE148_EN,
-				QCA8327_PWS_PACKAGE148_EN);
+				val);
 		if (ret)
 			return ret;
 	}
@@ -2098,7 +2105,12 @@ static int qca8k_resume(struct device *d
 static SIMPLE_DEV_PM_OPS(qca8k_pm_ops,
 			 qca8k_suspend, qca8k_resume);
 
-static const struct qca8k_match_data qca832x = {
+static const struct qca8k_match_data qca8327 = {
+	.id = QCA8K_ID_QCA8327,
+	.reduced_package = true,
+};
+
+static const struct qca8k_match_data qca8328 = {
 	.id = QCA8K_ID_QCA8327,
 };
 
@@ -2107,7 +2119,8 @@ static const struct qca8k_match_data qca
 };
 
 static const struct of_device_id qca8k_of_match[] = {
-	{ .compatible = "qca,qca8327", .data = &qca832x },
+	{ .compatible = "qca,qca8327", .data = &qca8327 },
+	{ .compatible = "qca,qca8328", .data = &qca8328 },
 	{ .compatible = "qca,qca8334", .data = &qca833x },
 	{ .compatible = "qca,qca8337", .data = &qca833x },
 	{ /* sentinel */ },
--- a/drivers/net/dsa/qca8k.h
+++ b/drivers/net/dsa/qca8k.h
@@ -260,6 +260,7 @@ struct ar8xxx_port_status {
 
 struct qca8k_match_data {
 	u8 id;
+	bool reduced_package;
 };
 
 enum {
