// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7242.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "avm,fritz300e", "qca,ar7242";
	model = "AVM FRITZ!WLAN Repeater 300E";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &ath9k;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		lan {
			label = "green:lan";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "green:wlan";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		rssi0 {
			label = "green:rssi0";
			gpios = <&ath9k 10 GPIO_ACTIVE_LOW>;
		};

		rssi1 {
			label = "green:rssi1";
			gpios = <&ath9k 4 GPIO_ACTIVE_LOW>;
		};

		rssi2 {
			label = "green:rssi2";
			gpios = <&ath9k 6 GPIO_ACTIVE_LOW>;
		};

		rssi3 {
			label = "green:rssi3";
			gpios = <&ath9k 7 GPIO_ACTIVE_LOW>;
		};

		rssi4 {
			label = "green:rssi4";
			gpios = <&ath9k 5 GPIO_ACTIVE_LOW>;
		};
	};

	eth-phy-reset {
		compatible = "regulator-fixed";

		regulator-name = "eth-phy-reset";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;

		gpio = <&gpio 11 GPIO_ACTIVE_LOW>;
		startup-delay-us = <300000>;
		enable-active-high;

		regulator-always-on;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x20000>;
				label = "urloader";
				read-only;
			};

			partition@20000 {
				compatible = "avm,eva-firmware";
				reg = <0x20000 0xee0000>;
				label = "firmware";
			};

			partition@f00000 {
				reg = <0xf00000 0x80000>;
				label = "tffs (1)";
				read-only;
			};

			partition@f80000 {
				reg = <0xf80000 0x80000>;
				label = "tffs (2)";
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		#gpio-cells = <2>;
		gpio-controller;
		qca,no-eeprom;
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "rgmii";
	};
};

&eth0 {
	status = "okay";

	phy-mode = "rgmii";
	phy-handle = <&phy0>;

	pll-data = <0x16000000 0x00000101 0x00001313>;
};
