// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7100.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "netgear,wndap360", "qca,ar7161";
	model = "Netgear WNDAP360";

	aliases {
		led-boot = &led_power_orange;
		led-failsafe = &led_power_orange;
		led-running = &led_power_orange;
		led-upgrade = &led_power_orange;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-output-names = "ref";
		clock-frequency = <40000000>;
	};

	leds {
		compatible = "gpio-leds";

		led_power_orange: power_orange {
			label = "orange:power";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wifi_2g_green {
			label = "green:wlan2g";
			gpios = <&ath9k0 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wifi_5g_green {
			label = "green:wlan5g";
			gpios = <&ath9k1 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0x0f>;
	phy1: ethernet-phy@1 {
		reg = <0x1>;
	};
};

&eth0 {
	status = "okay";

	phy-mode = "rgmii";
	phy-handle = <&phy1>;

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x010000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x790000>;
			};

			partition@7e0000 {
				label = "nvram";
				reg = <0x7e0000 0x010000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&pcie0 {
	status = "okay";

	ath9k0: wifi@0,11 {
		compatible = "pci168c,0029";
		reg = <0x8800 0 0 0 0>;
		qca,no-eeprom;
		nvmem-cells = <&macaddr_art_120c>;
		nvmem-cell-names = "mac-address";
		#gpio-cells = <2>;
		gpio-controller;
	};

	ath9k1: wifi@0,12 {
		compatible = "pci168c,0029";
		reg = <0x9000 0 0 0 0>;
		qca,no-eeprom;
		nvmem-cells = <&macaddr_art_520c>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <1>;
		#gpio-cells = <2>;
		gpio-controller;
	};
};


&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};

	macaddr_art_120c: macaddr@120c {
		reg = <0x120c 0x6>;
	};

	macaddr_art_520c: macaddr@520c {
		reg = <0x520c 0x6>;
	};
};
