From d44fd8604a4ab92119adb35f05fd87612af722b5 Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Sun, 19 Sep 2021 18:28:17 +0200
Subject: net: phy: at803x: fix spacing and improve name for 83xx phy

Fix spacing and improve name for 83xx phy following other phy in the
same driver.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/at803x.c | 60 ++++++++++++++++++++++++------------------------
 1 file changed, 30 insertions(+), 30 deletions(-)

--- a/drivers/net/phy/at803x.c
+++ b/drivers/net/phy/at803x.c
@@ -1318,47 +1318,47 @@ static struct phy_driver at803x_driver[]
 	.config_aneg		= at803x_config_aneg,
 }, {
 	/* QCA8337 */
-	.phy_id = QCA8337_PHY_ID,
-	.phy_id_mask = QCA8K_PHY_ID_MASK,
-	.name = "QCA PHY 8337",
+	.phy_id			= QCA8337_PHY_ID,
+	.phy_id_mask		= QCA8K_PHY_ID_MASK,
+	.name			= "Qualcomm Atheros 8337 internal PHY",
 	/* PHY_GBIT_FEATURES */
-	.probe = at803x_probe,
-	.flags = PHY_IS_INTERNAL,
-	.config_init = qca83xx_config_init,
-	.soft_reset = genphy_soft_reset,
-	.get_sset_count = at803x_get_sset_count,
-	.get_strings = at803x_get_strings,
-	.get_stats = at803x_get_stats,
+	.probe			= at803x_probe,
+	.flags			= PHY_IS_INTERNAL,
+	.config_init		= qca83xx_config_init,
+	.soft_reset		= genphy_soft_reset,
+	.get_sset_count		= at803x_get_sset_count,
+	.get_strings		= at803x_get_strings,
+	.get_stats		= at803x_get_stats,
 	.suspend		= genphy_suspend,
 	.resume			= genphy_resume,
 }, {
 	/* QCA8327-A from switch QCA8327-AL1A */
-	.phy_id = QCA8327_A_PHY_ID,
-	.phy_id_mask = QCA8K_PHY_ID_MASK,
-	.name = "QCA PHY 8327-A",
+	.phy_id			= QCA8327_A_PHY_ID,
+	.phy_id_mask		= QCA8K_PHY_ID_MASK,
+	.name			= "Qualcomm Atheros 8327-A internal PHY",
 	/* PHY_GBIT_FEATURES */
-	.probe = at803x_probe,
-	.flags = PHY_IS_INTERNAL,
-	.config_init = qca83xx_config_init,
-	.soft_reset = genphy_soft_reset,
-	.get_sset_count = at803x_get_sset_count,
-	.get_strings = at803x_get_strings,
-	.get_stats = at803x_get_stats,
+	.probe			= at803x_probe,
+	.flags			= PHY_IS_INTERNAL,
+	.config_init		= qca83xx_config_init,
+	.soft_reset		= genphy_soft_reset,
+	.get_sset_count		= at803x_get_sset_count,
+	.get_strings		= at803x_get_strings,
+	.get_stats		= at803x_get_stats,
 	.suspend		= genphy_suspend,
 	.resume			= genphy_resume,
 }, {
 	/* QCA8327-B from switch QCA8327-BL1A */
-	.phy_id = QCA8327_B_PHY_ID,
-	.phy_id_mask = QCA8K_PHY_ID_MASK,
-	.name = "QCA PHY 8327-B",
+	.phy_id			= QCA8327_B_PHY_ID,
+	.phy_id_mask		= QCA8K_PHY_ID_MASK,
+	.name			= "Qualcomm Atheros 8327-B internal PHY",
 	/* PHY_GBIT_FEATURES */
-	.probe = at803x_probe,
-	.flags = PHY_IS_INTERNAL,
-	.config_init = qca83xx_config_init,
-	.soft_reset = genphy_soft_reset,
-	.get_sset_count = at803x_get_sset_count,
-	.get_strings = at803x_get_strings,
-	.get_stats = at803x_get_stats,
+	.probe			= at803x_probe,
+	.flags			= PHY_IS_INTERNAL,
+	.config_init		= qca83xx_config_init,
+	.soft_reset		= genphy_soft_reset,
+	.get_sset_count		= at803x_get_sset_count,
+	.get_strings		= at803x_get_strings,
+	.get_stats		= at803x_get_stats,
 	.suspend		= genphy_suspend,
 	.resume			= genphy_resume,
 }, };
