// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Device Tree file for ESPRESSObin-Ultra
 * Copyright (C) 2019 Globalscale technologies, Inc.
 *
 * Jason Hung <jhung@globalscaletechnologies.com>
 */

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include "armada-372x.dtsi"

/ {
	model = "Globalscale Marvell ESPRESSOBin Ultra Board";
	compatible = "globalscale,espressobin-ultra", "marvell,armada3720",
		     "marvell,armada3710";

	aliases {
		/* for dsa slave device */
		ethernet1 = &switch0port1;
		ethernet2 = &switch0port2;
		ethernet3 = &switch0port3;
		ethernet4 = &switch0port4;
		ethernet5 = &switch0port5;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	memory@0 {
		device_type = "memory";
		reg = <0x00000000 0x00000000 0x00000000 0x20000000>;
	};

	reg_usb3_vbus: usb3-vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb3-vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
		gpio = <&gpionb 19 GPIO_ACTIVE_HIGH>;
	};

	usb3_phy: usb3-phy {
		compatible = "usb-nop-xceiv";
		vcc-supply = <&reg_usb3_vbus>;
	};

	leds {
		pinctrl-names = "default";
		compatible = "gpio-leds";
		/* No assigned functions to the LEDs by default */
		led1 {
			label = "ebin-ultra:blue:led1";
			gpios = <&gpionb 11 GPIO_ACTIVE_LOW>;
		};
		led2 {
			label = "ebin-ultra:green:led2";
			gpios = <&gpionb 12 GPIO_ACTIVE_LOW>;
		};
		led3 {
			label = "ebin-ultra:red:led3";
			gpios = <&gpionb 13 GPIO_ACTIVE_LOW>;
		};
		led4 {
			label = "ebin-ultra:yellow:led4";
			gpios = <&gpionb 14 GPIO_ACTIVE_LOW>;
		};
	};
};

&pcie0 {
	status = "okay";
};

&sata {
	status = "okay";
};

&sdhci0 {
	status = "okay";
	non-removable;
	bus-width = <8>;
	mmc-ddr-1_8v;
	mmc-hs400-1_8v;
	marvell,pad-type = "fixed-1-8v";
};

&spi0 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&spi_quad_pins>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <108000000>;
		spi-rx-bus-width = <4>;
		spi-tx-bus-width = <4>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "firmware";
				reg = <0x0 0x3e0000>;
			};
			partition@3e0000 {
				label = "hw-info";
				reg = <0x3e0000 0x10000>;
				read-only;
			};
			partition@3f0000 {
				label = "u-boot-env";
				reg = <0x3f0000 0x10000>;
			};
		};
	};
};

&uart0 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_pins>;
};

&i2c0 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2c1_pins>;

	clock-frequency = <100000>;

	rtc@51 {
		compatible = "nxp,pcf8563";
		reg = <0x51>;
	};
};

&usb3 {
	status = "okay";
	usb-phy = <&usb3_phy>;
};

&usb2 {
	status = "okay";
};

&eth0 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii_pins>;
	phy-mode = "rgmii-id";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&mdio {
	status = "okay";

	extphy: ethernet-phy@0 {
		reg = <1>;
	};

	switch0: switch0@1 {
		compatible = "marvell,mv88e6085";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <3>;

		dsa,member = <0 0>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			switch0port0: port@0 {
				reg = <0>;
				label = "cpu";
				ethernet = <&eth0>;
			};

			switch0port1: port@1 {
				reg = <1>;
				label = "lan0";
				phy-handle = <&switch0phy1>;
			};

			switch0port2: port@2 {
				reg = <2>;
				label = "lan1";
				phy-handle = <&switch0phy2>;
			};

			switch0port3: port@3 {
				reg = <3>;
				label = "lan2";
				phy-handle = <&switch0phy3>;
			};

			switch0port4: port@4 {
				reg = <4>;
				label = "lan3";
				phy-handle = <&switch0phy4>;
			};

			switch0port5: port@5 {
				reg = <5>;
				label = "wan";
				phy-handle = <&extphy>;
				phy-mode = "sgmii";
			};
		};

		mdio {
			#address-cells = <1>;
			#size-cells = <0>;

			switch0phy1: switch0phy1@11 {
				reg = <0x11>;
			};
			switch0phy2: switch0phy2@12 {
				reg = <0x12>;
			};
			switch0phy3: switch0phy3@13 {
				reg = <0x13>;
			};
			switch0phy4: switch0phy4@14 {
				reg = <0x14>;
			};
		};
	};
};
