// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Ubiquiti UniFi AP Pro";
	compatible = "ubnt,unifi-ap-pro";

	aliases {
		led-boot = &led_white;
		led-failsafe = &led_white;
		led-running = &led_blue;
		led-upgrade = &led_blue;
		label-mac-device = &eth0;
	};

	leds {
		compatible = "gpio-leds";

		led_white: led-white {
			label = "white:dome";
			gpios = <&gpio 12 GPIO_ACTIVE_HIGH>;
		};

		led_blue: led-blue {
			label = "blue:dome";
			gpios = <&gpio 13 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "firmware";
				reg = <0x50000 0xf60000>;

				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					label = "kernel";
					reg = <0x0 0x300000>;
					/* Can be resized w/o issues.
					 * U-Boot can load kernel from the
					 * entirety of the "firmware" partition space.
					 */
				};

				partition@300000 {
					label = "rootfs";
					reg = <0x300000 0xc60000>;
				};
			};

			partition@fb0000 {
				label = "cfg";
				reg = <0xfb0000 0x40000>;
				read-only;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "pci168c,0033";
		reg = <0 0 0 0 0>;
		qca,no-eeprom;
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;

		qca,ar8327-initvals = <
			0x4 0x7600000 /* PORT0 PAD MODE CTRL */
			0x10 0x80000080 /* POWER_ON_STRAP */
			0x7c 0x7e /* PORT0_STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x6000000 0x101 0x1616>;

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";

	phy-mode = "rgmii";
	phy-handle = <&phy0>;
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
