--- a/drivers/mtd/spi-nor/xmc.c
+++ b/drivers/mtd/spi-nor/xmc.c
@@ -14,6 +14,8 @@ static const struct flash_info xmc_parts
 			    SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 	{ "XM25QH128A", INFO(0x207018, 0, 64 * 1024, 256,
 			     SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
+	{ "XM25QH128C", INFO(0x204018, 0, 64 * 1024, 256,
+			     SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 };
 
 const struct spi_nor_manufacturer spi_nor_xmc = {
