// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9330.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "D-Link DIR-505";
	compatible = "dlink,dir-505", "qca,ar9330";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_status_red;
		led-running = &led_power_green;
		led-upgrade = &led_status_red;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "WPS button";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "Reset button";
			gpios = <&gpio 12 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		led_power_green: power {
			label = "green:power";
			gpios = <&gpio 27 GPIO_ACTIVE_LOW>;
		};

		led_status_red: status {
			label = "red:status";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio {
	led_enable {
		gpio-hog;
		output-low;
		gpios = <1 GPIO_ACTIVE_LOW>;
		line-name = "d-link:power:led";
	};
};

&usb {
	dr_mode = "host";
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&eth0 {
	status = "okay";

	gmac-config {
		device = <&gmac>;
		switch-phy-addr-swap = <0>;
		switch-phy-swap = <0>;
	};
};

&eth1 {
	compatible = "syscon", "simple-mfd";
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <50000000>;
		reg = <0>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x10000>;
				read-only;
			};

			art: partition@10000 {
				label = "art";
				reg = <0x10000 0x10000>;
				read-only;
			};

			mac: partition@20000 {
				label = "mac";
				reg = <0x20000 0x10000>;
				read-only;
			};

			partition@30000 {
				label = "nvram";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "language";
				reg = <0x40000 0x40000>;
				read-only;
			};

			partition@80000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x80000 0x780000>;
			};
		};
	};
};

&wmac {
	status = "okay";
	qca,no-eeprom;
};
