#!/bin/sh
#
# Copyright (C) 2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/ar71xx.sh

board=$(ar71xx_board_name)

case "$board" in
nanostation-m)
	ucidef_set_gpio_switch "poe_passthrough" "PoE Passthrough" "2"
	;;
nanostation-m-xw)
	ucidef_set_gpio_switch "poe_passthrough" "PoE Passthrough" "8"
	;;
cpe510)
	ucidef_set_gpio_switch "poe_passthrough" "PoE Passthrough" "20"
	;;
esac

ucidef_commit_gpio_switches

exit 0
