--- a/arch/mips/ath79/mach-ubnt-xm.c
+++ b/arch/mips/ath79/mach-ubnt-xm.c
@@ -21,6 +21,8 @@
 #include <asm/mach-ath79/irq.h>
 #include <asm/mach-ath79/ar71xx_regs.h>
 
+#include <linux/platform_data/phy-at803x.h>
+
 #include "common.h"
 #include "dev-ap9x-pci.h"
 #include "dev-eth.h"
@@ -404,6 +406,40 @@ static struct gpio_led ubnt_xw_leds_gpio
 	},
 };
 
+#define UBNT_ROCKET_TI_GPIO_LED_L1	16
+#define UBNT_ROCKET_TI_GPIO_LED_L2	17
+#define UBNT_ROCKET_TI_GPIO_LED_L3	18
+#define UBNT_ROCKET_TI_GPIO_LED_L4	19
+#define UBNT_ROCKET_TI_GPIO_LED_L5	20
+#define UBNT_ROCKET_TI_GPIO_LED_L6	21
+static struct gpio_led ubnt_rocket_ti_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt:green:link1",
+		.gpio		= UBNT_ROCKET_TI_GPIO_LED_L1,
+		.active_low	= 1,
+	}, {
+		.name		= "ubnt:green:link2",
+		.gpio		= UBNT_ROCKET_TI_GPIO_LED_L2,
+		.active_low	= 1,
+	}, {
+		.name		= "ubnt:green:link3",
+		.gpio		= UBNT_ROCKET_TI_GPIO_LED_L3,
+		.active_low	= 1,
+	}, {
+		.name		= "ubnt:green:link4",
+		.gpio		= UBNT_ROCKET_TI_GPIO_LED_L4,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt:green:link5",
+		.gpio		= UBNT_ROCKET_TI_GPIO_LED_L5,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt:green:link6",
+		.gpio		= UBNT_ROCKET_TI_GPIO_LED_L6,
+		.active_low	= 0,
+	},
+};
+
 static void __init ubnt_xw_init(void)
 {
 	u8 *eeprom = (u8 *) KSEG1ADDR(0x1fff0000);
@@ -477,6 +513,62 @@ static void __init ubnt_rocket_m_xw_setu
 	ath79_register_eth(0);
 }
 
+static struct at803x_platform_data ubnt_rocket_m_ti_at803_data = {
+	.disable_smarteee = 1,
+	.enable_rgmii_rx_delay = 1,
+	.enable_rgmii_tx_delay = 1,
+};
+static struct mdio_board_info ubnt_rocket_m_ti_mdio_info[] = {
+        {
+                .bus_id = "ag71xx-mdio.0",
+                .phy_addr = 4,
+                .platform_data = &ubnt_rocket_m_ti_at803_data,
+        },
+};
+
+static void __init ubnt_rocket_m_ti_setup(void)
+{
+	u8 *eeprom = (u8 *) KSEG1ADDR(0x1fff0000);
+
+	ath79_register_m25p80(NULL);
+
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_rocket_ti_leds_gpio),
+				 ubnt_rocket_ti_leds_gpio);
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+                                        ARRAY_SIZE(ubnt_xm_gpio_keys),
+                                        ubnt_xm_gpio_keys);
+
+	ap91_pci_init(eeprom + 0x1000, NULL);
+
+	ath79_setup_ar934x_eth_cfg(AR934X_ETH_CFG_RGMII_GMAC0);
+	ath79_setup_ar934x_eth_rx_delay(3, 3);
+	ath79_init_mac(ath79_eth0_data.mac_addr,
+		       eeprom + UAP_PRO_MAC0_OFFSET, 0);
+	ath79_init_mac(ath79_eth1_data.mac_addr,
+		       eeprom + UAP_PRO_MAC1_OFFSET, 0);
+
+	ath79_eth0_data.phy_if_mode = PHY_INTERFACE_MODE_RGMII;
+	ath79_eth0_data.mii_bus_dev = &ath79_mdio0_device.dev;
+	ath79_eth1_data.phy_if_mode = PHY_INTERFACE_MODE_GMII;
+	ath79_eth1_data.mii_bus_dev = &ath79_mdio1_device.dev;
+	
+	mdiobus_register_board_info(ubnt_rocket_m_ti_mdio_info,
+			ARRAY_SIZE(ubnt_rocket_m_ti_mdio_info));
+	ath79_register_mdio(0, 0x0);
+
+
+	ath79_eth0_data.phy_mask = BIT(4);
+	/* read out from vendor */
+	ath79_eth0_pll_data.pll_1000 = 0x2000000;
+	ath79_eth0_pll_data.pll_10 = 0x1313;
+	ath79_register_eth(0);
+
+	ath79_register_mdio(1, 0x0);
+	ath79_eth1_data.phy_mask = BIT(3);
+	ath79_register_eth(1);
+}
+
+
 MIPS_MACHINE(ATH79_MACH_UBNT_NANO_M_XW, "UBNT-NM-XW", "Ubiquiti Nanostation M XW",
 	     ubnt_nano_m_xw_setup);
 
@@ -486,6 +578,9 @@ MIPS_MACHINE(ATH79_MACH_UBNT_LOCO_M_XW,
 MIPS_MACHINE(ATH79_MACH_UBNT_ROCKET_M_XW, "UBNT-RM-XW", "Ubiquiti Rocket M XW",
 	     ubnt_rocket_m_xw_setup);
 
+MIPS_MACHINE(ATH79_MACH_UBNT_ROCKET_M_TI, "UBNT-RM-TI", "Ubiquiti Rocket M TI",
+	     ubnt_rocket_m_ti_setup);
+
 static struct gpio_led ubnt_airgateway_gpio_leds[] __initdata = {
 	{
 		.name	   = "ubnt:blue:wlan",
--- a/arch/mips/ath79/machtypes.h
+++ b/arch/mips/ath79/machtypes.h
@@ -178,6 +178,7 @@ enum ath79_mach_type {
 	ATH79_MACH_UBNT_NANO_M_XW, 	/* Ubiquiti NanoStation M XW */
 	ATH79_MACH_UBNT_ROCKET_M,	/* Ubiquiti Rocket M */
 	ATH79_MACH_UBNT_ROCKET_M_XW,	/* Ubiquiti Rocket M XW*/
+	ATH79_MACH_UBNT_ROCKET_M_TI,	/* Ubiquiti Rocket M TI*/
 	ATH79_MACH_UBNT_RSPRO,		/* Ubiquiti RouterStation Pro */
 	ATH79_MACH_UBNT_RS,		/* Ubiquiti RouterStation */
 	ATH79_MACH_UBNT_UAP_PRO,	/* Ubiquiti UniFi AP Pro */
