From fc300dc3733fdc328e6e10c7b8379b60c26cd648 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Fri, 20 Mar 2015 23:14:32 +0100
Subject: [PATCH] bgmac: allow enabling on ARCH_BCM_5301X
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Home routers based on ARM SoCs like BCM4708 also have bcma bus with core
supported by bgmac.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/broadcom/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/broadcom/Kconfig
+++ b/drivers/net/ethernet/broadcom/Kconfig
@@ -142,7 +142,7 @@ config BNX2X_SRIOV
 
 config BGMAC
 	tristate "BCMA bus GBit core support"
-	depends on BCMA_HOST_SOC && HAS_DMA && BCM47XX
+	depends on BCMA_HOST_SOC && HAS_DMA && (BCM47XX || ARCH_BCM_5301X)
 	select PHYLIB
 	---help---
 	  This driver supports GBit MAC and BCM4706 GBit MAC cores on BCMA bus.
